;; Realtek 10/100/1000 PCI-E NIC Family all in one NDIS Driver
;;
;; Copyright 2009, Realtek Semiconductor Corporation.
;;
;; This product is covered by one or more of the following patents:
;; US5,307,459, US5,434,872, US5,732,094, US6,570,884, US6,115,776, 
;; and US6,327,625.
;;
;; This release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                               
CatalogFile.NT = netrtle.cat                        ;;for WHQL certified
DriverVer      = 06/04/2009,5.728.0604.2009

[Manufacturer]
%Realtek%      = Realtek, NTx86.5.1, NTamd64

[ControlFlags]
ExcludeFromSelect = *

[Realtek]
; DisplayName            Section            DeviceID
; -----------            -------            --------
;8101E
%RTL8136.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01
;8131
%RTL8131.DeviceDesc%    = RTL8136.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_83A01043&REV_01

;8101HP
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HP.ndi,    PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;8102E/8103E
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02

;8104E
%RTL8104.DeviceDesc%    = RTL8104.ndi,      PCI\VEN_10EC&DEV_8137&REV_03
%RTL8104.DeviceDesc%    = RTL8104.ndi,      PCI\VEN_10EC&DEV_8137&SUBSYS_813710EC&REV_03

;8401E
%RTL8401.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&REV_04
%RTL8401.DeviceDesc%    = RTL8102.ndi,      PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_04

;8168B
%RTL8168.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01
;8112
%RTL8112.DeviceDesc%    = RTL8168.ndi,      PCI\VEN_10EC&DEV_8168&SUBSYS_83851043&REV_01

;8168C
%RTL8168C.DeviceDesc%   = RTL8168C.ndi,     PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168C.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS
;8168CForceGigabit
%RTL8168C.DeviceDesc%   = RTL8168CForceGigabit.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_83AB1043&REV_02 ;ASUS
;8168CMitac
%RTL8168C.DeviceDesc%   = RTL8168CMitac.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_92131071&REV_02 ;Mitac

;8168D
%RTL8168D.DeviceDesc%   = RTL8168D.ndi,     PCI\VEN_10EC&DEV_8168&REV_03
%RTL8168D.DeviceDesc%   = RTL8168D.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_03
;8112L
%RTL8112L.DeviceDesc%   = RTL8168D.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_83A31043&REV_03

; 8168DP
%RTL8168DP.DeviceDesc%  = RTL8168DP.ndi,    PCI\VEN_10EC&DEV_8168&REV_04
%RTL8168DP.DeviceDesc%  = RTL8168DP.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_04

[Realtek.NTx86.5.1]; This section will only be installed by Windows XP
;8101E
%RTL8136.DeviceDesc%	= RTL8136x.ndi,	    PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%	= RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_180E147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_240F147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_010C1025&REV_01 ;ACER
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_026C1025&REV_01 ;ACER
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_26721025&REV_01 ;ACER
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_B10A1897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_BC891897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_BD891897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0618A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_063DA0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0631A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0634A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0636A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0640A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2055161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206A161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206B161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0560107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0561107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0565107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0566107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F51043&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F61043&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10A1631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2101631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2121631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_53498086&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_D6068086&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001940&REV_01 ;Channel
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_027D1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_027E1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02AD1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B41028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F821019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F961019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81361019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90A21019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_906B1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AC1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B11019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90371695&REV_01 ;Epox
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_601F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60251509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60291509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60401509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60411509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60421509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60431509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60441509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60451509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60461509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60471509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60481509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60491509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604B1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604C1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604D1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604E1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C40105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C76105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CF7105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D43105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D44105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4A105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4B105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4F105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DD6105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DDA105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE9105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DEA105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DED105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DEE105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0E19105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11231734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0380107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0381107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0386107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001458&REV_01 ;Gigabyte
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10128086&REV_01 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_D6078086&REV_01 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00161170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00371170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00411170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813616F3&REV_01 ;JETWAY
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_301A17AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_302917AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_303017AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01151854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01161854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_20001854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_20011854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_82521071&REV_01 ;MiTAC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_276C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_302C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_313C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_314C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_327C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_337C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_367C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_368C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_369C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_373C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_376C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_379C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_382C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_387C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_43401462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_44101462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_501C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_525C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_528C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_536C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_63F11462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_63F61462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_66101462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732A1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732B1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_75261462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_75351462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_75651462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_75691462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10271631&REV_01 ;NEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C0271631&REV_01 ;NEC
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10C1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10D1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0311631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E03B1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01991025&REV_01 ;PEGATRON
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_200C1B0A&REV_01 ;PEGATRON
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0368107B&REV_01 ;RT-QTA
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_B05F144D&REV_01 ;SAMSUNG
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_104D13BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105213BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105313BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105413BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_01 ;Toshiba(Compal)
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF011179&REV_01 ;Toshiba(Compal)
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00011179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF311179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF501179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2B301584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_97001584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A01414FF&REV_01 ;WHITE BOX
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2161631&REV_01 ;Wistron
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_113A1734&REV_01 ;Wistron
%RTL8136.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0&REV_01 ;Wistron
;8131
%RTL8131.DeviceDesc%    = RTL8136x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_83A01043&REV_01

;8101HP
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A89103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPx.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;8102E/8103E
%RTL8102.DeviceDesc%	= RTL8102x.ndi,	    PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0300196F&REV_02 ;AVG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_015A1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_015B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_017B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_019B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02441025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02551025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02561025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02661025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02761025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_028C1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_03011025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_064BA0A0&REV_02 ;AOPEN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_059817FF&REV_02 ;BenQ
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_059A17FF&REV_02 ;BenQ
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_059B17FF&REV_02 ;BenQ
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_059C17FF&REV_02 ;BenQ
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01301558&REV_02 ;Channel
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_08901558&REV_02 ;Channel
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_71201558&REV_02 ;Channel
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0184107B&REV_02 ;COMPAL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02741028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02971028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02981028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02991028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_029A1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02A91028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02AD1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B01028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B21028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B41028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B51028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B81028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02C61028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02CB1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02CC1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02CF1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02DF1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02E01028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02E11028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02E21028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02F41028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02FA1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_040E1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_041A1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81021019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81031019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_82481019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_83481019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90871019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90891019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90921019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90931019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90941019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90951019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90961019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B31019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B41019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B51019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B61019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B71019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B91019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90BA1019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_99701019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_99B51019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A1001019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50011509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50021509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50031509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50041509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50051509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80201509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80211509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80221509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CF7105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4B105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DC0105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DC1105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DD6105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DDA105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE9105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DEA105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DED105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DEE105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF2105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF6105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF7105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0E19105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11601734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11611734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_118D1734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_118E1734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_153410CF&REV_02 ;FUJI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_153510CF&REV_02 ;FUJI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_40021B0A&REV_02 ;HAIER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_40091B0A&REV_02 ;HAIER
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A85103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A88103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A8A103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A8C103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A97103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A98103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A9D103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3054103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3055103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3059103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3060103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3061103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3062103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3063103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3064103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3069103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_306A103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_306B103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_306C103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_306D103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30DE103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30F2103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30F3103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30F7103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30FB103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30FE103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3600103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3602103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3603103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3607103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_360B103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3621103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3622103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3623103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3627103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3635103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3636103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3637103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3638103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3639103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363A103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363B103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363C103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363D103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363E103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363F103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3642103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3643103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3644103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3649103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3650103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3652103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3656103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3657103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_7010103C ;HP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00051170&REV_02 ;INVENTEC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_219D17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_389E17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17721854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17731854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17741854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17751854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17761854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17791854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17801854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17811854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17821854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17831854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17841854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17851854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17861854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17871854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17881854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17891854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17901854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00021B7D&REV_02 ;MALATA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A0291071&REV_02 ;MITAC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_74001057&REV_02 ;MOTOROLA
;%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01101462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_100A1462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10171462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_101E1462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10271462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10281462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_102B1462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10311462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_88FA1033&REV_02 ;NEC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_890F1033&REV_02 ;NEC
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_018B1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_018C1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01931631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2141631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2151631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2181631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2191631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2161631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2171631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2181631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2191631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E21B1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_201F1B0A&REV_02 ;PEGATRON
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0772152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0773152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0774152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0775152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0776152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0777152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0778152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0779152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0780152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0781152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0782152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0783152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0784152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0785152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0786152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0787152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0788152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0789152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1777152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_B05F144D&REV_02 ;SAMSUNG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_B065144D&REV_02 ;SAMSUNG
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105713BD&REV_02 ;SHARP
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602A1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602B1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602C1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602D1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602E1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602F1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60301509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60311509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60321509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60331509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60341509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60351509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60361509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60371509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60381509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60391509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603A1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603B1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603C1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603D1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603E1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603F1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00021179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00031179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1F1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF401179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF641179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF661179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF671179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF681179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF6A1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FFC01179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003014C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003114C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003214C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003314C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003414C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003514C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003614C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003714C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003C14C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003D14C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003E14C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_004614C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_004814C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_004914C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A01414FF&REV_02 ;WHITE BOX
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2161631&REV_02 ;WISTRON
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_113A1734&REV_02 ;WISTRON
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0&REV_02 ;WISTRON
%RTL8102.DeviceDesc%	= RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10C617C0&REV_02 ;WISTRON

;8104E
%RTL8104.DeviceDesc%    = RTL8104x.ndi,     PCI\VEN_10EC&DEV_8137&REV_03
%RTL8104.DeviceDesc%    = RTL8104x.ndi,     PCI\VEN_10EC&DEV_8137&SUBSYS_813710EC&REV_03

;8401E
%RTL8401.DeviceDesc%    = RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&REV_04
%RTL8401.DeviceDesc%    = RTL8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_04

;8168B
%RTL8168.DeviceDesc%	= RTL8168x.ndi,	    PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1071147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1072147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1073147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1074147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1077147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1078147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1079147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_107A147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_240D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2410147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2412147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01071025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_010C1025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01261025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_26511025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0B105B&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B1331897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B2201897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_060DA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0611A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0614A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0616A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061BA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061CA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0623A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0624A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0625A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_063EA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0642A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2055161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206A161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206B161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_11F51043&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1043&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001940&REV_01 ;Channel
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05211558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05911558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_09021558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002014C0&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002114C0&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_01 ;DELL
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_01 ;DELL
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F711019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F721019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F761019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F771019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F811019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F821019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_902A1019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90361695&REV_01 ;Epox
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_601F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60251509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60291509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801C1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801D1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801E1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C76105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7D105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C88105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C89105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C90105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C91105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C92105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE7105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D0E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D16105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF9105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D43105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D44105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D4C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE7105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE9105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DEA105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DEE105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DEF105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DFD105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E17105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E18105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E19105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_111C1734&REV_01 ;FSC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_01 ;FSC(D45/D46)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0690107B&REV_01 ;GATEWAY
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_01 ;Gigabyte
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30B6103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30CC103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_D6088086&REV_01 ;INTEL
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_00401170&REV_01 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_500E17FF&REV_01 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816816F3&REV_01 ;JETWAY
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_302917AA&REV_01 ;Lenovo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_303017AA&REV_01 ;Lenovo
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47011071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_82521071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B3001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03411462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05311462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_238C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_270C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_276C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_279C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_280C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2F811462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB31462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FBD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_309C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_327C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33201462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33371462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33411462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_334B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_337C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_338C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33FF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_34131462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_345C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_348C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_356C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_367C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_368C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_373C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_375C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_376C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_379C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_384C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_387C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3F711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB91462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FCC1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FD51462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FDF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF41462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FFE1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42CD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42D71462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42E11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43141462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43241462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43271462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_514C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63701462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63F21462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63F41462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_65101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_65301462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_71901462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_71F11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_72101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_72301462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_73271462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732A1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4121462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4221462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80111854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80161854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80171854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0151631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9011631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9021631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_83841033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_887E1033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_20021B0A&REV_01 ;PEGATRON
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_058F17FF&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0761152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0762152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0763152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B052144D&REV_01 ;SAMSUNG
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B057144D&REV_01 ;SAMSUNG
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_104D13BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF001179&REV_01 ;Toshiba(Compal)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF011179&REV_01 ;Toshiba(Compal)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10CD1734&REV_01 ;Uniwill(FSC)
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90761584&REV_01 ;Uniwill
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_110E1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10C317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A00D14FF&REV_01 ;XPLORE
;8112
%RTL8112.DeviceDesc%    = RTL8168x.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_83851043&REV_01

;8168C
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B2301897&REV_02 ;AMTEK
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_013E1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01401025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01441025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_014C1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01361025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_016D1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_016E1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02291025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02381025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_025F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02611025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_026F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02801025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02811025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02821025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02831025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02841025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02851025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02861025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02871025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02881025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02891025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_028A1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_028B1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03021025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03031025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03041025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_13601019&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_063AA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0643A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0644A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0646A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0648A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_064AA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_064EA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0700A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0703A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_234EA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03E91AA7&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_16D51043&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_C2111631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_C2131631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080017FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080117FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080217FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080317FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080517FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_090017FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_016B107B&REV_02 ;Compal
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_016D107B&REV_02 ;Compal
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_313C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_398C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_501C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_513C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_519C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_528C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75301462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75331462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75501462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75511462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_73751462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01261558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03901558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04811558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_072F1558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08051558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08061558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08601558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_09031558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_56011558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_70011558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76401558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76411558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02581028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_026F1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02731028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02751028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02791028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027D1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027E1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02821028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02831028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02851028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02A91028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02AC1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02B51028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02D91028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_81111019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90AD1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50011509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50021509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50031509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50041509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50051509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60421509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60431509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_80201509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_80211509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_80221509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_802C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D16105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D4C105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DDB105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DE7105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DE9105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DEA105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DEE105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DEF105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF0105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DFD105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E17105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E18105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E19105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E1C105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_11351734&REV_02 ;FSC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0900107B&REV_02 ;GATEWAY
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_1505103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_1506103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A6F103C&REV_02 ;HP cPC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A73103C&REV_02 ;HP bPC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A74103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A7F103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A80103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A82103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A85103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A88103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A8A103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2B00103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3038103C ;HP-CDC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_303A103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_303B103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3043103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3045103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30DE103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F1103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F2103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F4103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F7103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F8103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30FC103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30FB103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3600103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3602103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3603103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_360F103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3610103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_361B103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_361C103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_361D103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_361E103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3621103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3622103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3624103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3628103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3629103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3633103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_7010103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_000E1B0A&REV_02 ;HAIER
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_001F1B0A&REV_02 ;HAIER(EPSON)
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6098086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6128086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_011F1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01201854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01211854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01221854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17721854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17731854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17741854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17751854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17761854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17791854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17801854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17881854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17891854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_20021854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_20031854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_20071854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10051462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10081462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10181462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_22701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_392C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_43201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_43501462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_43701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_43801462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_515C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_520C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_522C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_536C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_63F51462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_65201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_65101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67401462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_71F01462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_72201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_73881462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75121462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75161462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75221462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75261462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75321462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75351462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75431462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75461462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75491462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75521462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75581462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75641462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75661462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75691462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75721462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75931462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A1101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_83691033&REV_02 ;NEC
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00031B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_006A1B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_200B1B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0772152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0773152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0774152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0775152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0776152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0777152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0779152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0780152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B04E144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B052144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B057144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B063144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00201B0A&REV_02 ;SI
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602A1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602B1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602C1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602D1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602E1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602F1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60301509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60311509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60321509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60331509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60341509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60351509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60361509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60371509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60381509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60391509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603A1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603B1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603C1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603D1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603E1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603F1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60401509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60421509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60431509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_82E919DB&REV_02 ;TCL
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_210817AA&REV_02 ;THINKPAD
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00091290&REV_02 ;TOPS
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60341991&REV_02 ;TOPSTAR
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00011179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1F1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF671179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF7A1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_109C147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_1102147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_1103147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003014C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003114C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003214C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003314C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003414C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003514C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003614C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003714C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003914C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003C14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003D14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003E14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A00C14FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A01514FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A01614FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A02014FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_11631734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10C017C0&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_409017C0&REV_02 ;WISTRON
;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUSx.ndi,PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS
;8168CForceGigabit
%RTL8168C.DeviceDesc%   = RTL8168CForceGigabitx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_83AB1043&REV_02 ;ASUS
;8168CMitac
%RTL8168C.DeviceDesc%   = RTL8168CMitacx.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_92131071&REV_02 ;Mitac

;8168D
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&REV_03
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_03
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_024E1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_024F1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_025A1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02661025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02761025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0700A0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_16D51043&REV_03 ;ASUS
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080417FF&REV_03 ;BENQ
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01301558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_86871558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_86891558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02BA1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02BB1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02BC1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02BD1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02C01028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02D81028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02EA1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02EB1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02F21028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02F51028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04011028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04021028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04031028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04081028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04151028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04161028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04181028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_041E1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_041F1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_811D1019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_8D481019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90931019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90B61019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90B71019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_400A1B0A&REV_03 ;
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DC0105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DC1105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DD4105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF2105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF6105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF7105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E0C105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E0D105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_118D1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_118E1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0256103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A8E103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A90103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A92103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A94103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A97103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A9C103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3046103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3059103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3060103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3061103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3062103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3063103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3064103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_306D103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3635103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3636103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3637103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3638103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3639103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363B103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363C103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363D103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363E103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363F103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3652103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_7001103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00671170&REV_03 ;INVENTEC
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6138086&REV_03 ;INTEL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6148086&REV_03 ;INTEL
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_213117AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_210817AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_306917AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_38A017AA&REV_03 ;LENOVO
;%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17811854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17821854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17831854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17841854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17851854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17861854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17871854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_92231071&REV_03 ;MITAC
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_92701071&REV_03 ;MITAC
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_74001057&REV_03 ;MOTOROLA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10041462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10061462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10081462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_100E1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_100F1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10111462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10121462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_101C1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_101D1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_101F1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10201462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10211462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10221462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_102D1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75261462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75631462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75741462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75761462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75771462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75791462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75801462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75811462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75861462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75871462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75921462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75951462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75961462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75991462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76021462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76091462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_12021849&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_15011849&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_20221B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0784152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0785152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0786152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0787152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0788152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0789152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00021179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1E1179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1F1179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF401179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FFC01179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_004614C0&REV_03 ;WB
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_004814C0&REV_03 ;WB
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_004914C0&REV_03 ;WB
%RTL8168D.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10CB17C0&REV_03 ;WISTRON



;8112L
%RTL8112L.DeviceDesc%   = RTL8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_83A31043&REV_03

; 8168DP
%RTL8168DP.DeviceDesc%  = RTL8168DPx.ndi,   PCI\VEN_10EC&DEV_8168&REV_04
%RTL8168DP.DeviceDesc%  = RTL8168DPx.ndi,   PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_04

;PNP_CHG_XP32
%RTL8102.DeviceDesc%	= RTLChgPnpCaps8102x.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17721854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17731854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17741854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17751854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17761854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17791854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17801854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17881854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Cx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17891854&REV_02 ;LGE
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17811854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17821854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17831854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17841854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17851854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17861854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Dx.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17871854&REV_03 ;LG

[Realtek.NTamd64]; This section will only be installed by Windows XP 64-bit
;8101E
%RTL8136.DeviceDesc%	= RTL8136a.ndi,	    PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%	= RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_180E147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_240F147B&REV_01 ;ABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_010C1025&REV_01 ;ACER
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_026C1025&REV_01 ;ACER
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_26721025&REV_01 ;ACER
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_B10A1897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_BC891897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_BD891897&REV_01 ;AMTEK
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0618A0A0&REV_01 ;AOpen
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_063DA0A0&REV_01 ;AOPEN
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2055161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206A161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_206B161F&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0560107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0561107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0565107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0566107B&REV_01 ;Arima
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F51043&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_12F61043&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10A1631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2101631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2121631&REV_01 ;ASUS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001940&REV_01 ;Channel
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_027D1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_027E1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02AD1028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B41028&REV_01 ;DELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F821019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0F961019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81361019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_902A1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_906B1019&REV_01 ;ECS(INTEL)
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AC1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B11019&REV_01 ;ECS
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90371695&REV_01 ;Epox
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_601F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60251509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60291509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60401509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60411509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60421509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60431509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60441509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60451509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60461509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60471509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60481509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60491509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604A1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604B1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604C1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604D1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604E1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_604F1509&REV_01 ;FIC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C40105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0C76105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CF7105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D43105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D44105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4A105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4B105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4F105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DD6105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DDA105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE9105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DEA105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DED105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DEE105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0E19105B&REV_01 ;Foxconn
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11231734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_01 ;FSC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0380107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0381107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0386107B&REV_01 ;GATEWAY
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0001458&REV_01 ;GBT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10128086&REV_01 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_D6078086&REV_01 ;INTEL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00161170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00371170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00411170&REV_01 ;INVENTEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813616F3&REV_01 ;JETWAY
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_301A17AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_302917AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_303017AA&REV_01 ;Lenovo
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01151854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01161854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_20001854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_20011854&REV_01 ;LGE
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_82521071&REV_01 ;MiTAC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_276C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_302C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_313C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_314C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_327C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_337C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_367C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_368C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_373C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_376C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_382C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_387C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_379C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_43401462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_44101462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_501C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_525C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_528C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_536C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_63F11462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_63F61462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_66101462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_501C1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732A1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_732B1462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_75261462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_75351462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_75651462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_75691462&REV_01 ;MSI
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10271631&REV_01 ;NEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C0271631&REV_01 ;NEC
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10C1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C10D1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E0311631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E03B1631&REV_01 ;PACKARDBELL
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01991025&REV_01 ;PEGATRON
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_200C1B0A&REV_01 ;PEGATRON
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0368107B&REV_01 ;RT-QTA
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_B05F144D&REV_01 ;SAMSUNG
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_104D13BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105213BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105313BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105413BD&REV_01 ;Sharp
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_01 ;Toshiba(Compal)
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF011179&REV_01 ;Toshiba(Compal)
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00011179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF311179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF501179&REV_01 ;Toshiba
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2B301584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_97001584&REV_01 ;Uniwill
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A01414FF&REV_01 ;WHITEBOX
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2161631&REV_01 ;Wistron
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_113A1734&REV_01 ;Wistron
%RTL8136.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0&REV_01 ;Wistron
;8131
%RTL8131.DeviceDesc%    = RTL8136a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_83A01043&REV_01

;8101HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A57103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A78103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A79103C ;HP-CPC
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_2A89103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_30CB103C ;HP
%RTL8136.DeviceDesc%    = RTL8136HPa.ndi,   PCI\VEN_10EC&DEV_8136&SUBSYS_FF101179&REV_01 ;Toshiba

;8102E/8103E
%RTL8102.DeviceDesc%	= RTL8102a.ndi,	    PCI\VEN_10EC&DEV_8136&REV_02
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0300196F&REV_02 ;AVG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_015A1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_015B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_017B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_019B1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02441025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02551025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02561025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02661025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02761025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_028C1025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_03011025&REV_02 ;ACER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_064BA0A0&REV_02 ;AOPEN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_059817FF&REV_02 ;BenQ
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_059A17FF&REV_02 ;BenQ
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_059B17FF&REV_02 ;BenQ
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_059C17FF&REV_02 ;BenQ
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01301558&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_08901558&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_71201558&REV_02 ;CHANNEL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0184107B&REV_02 ;COMPAL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02741028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02971028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02981028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02991028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_029A1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02A91028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02AD1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B01028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B21028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B41028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B51028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02B81028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02C61028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02CB1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02CC1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02CF1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02DF1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02E01028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02E11028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02E21028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02F41028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_02FA1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_040E1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_041A1028&REV_02 ;DELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81021019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_81031019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_82481019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_83481019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90871019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90891019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90921019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90931019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90941019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90951019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90961019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B31019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B41019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B51019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B61019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B71019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90B91019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_90BA1019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_99701019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_99B51019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A1001019&REV_02 ;ECS
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50011509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50021509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50031509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50041509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_50051509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80201509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80211509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_80221509&REV_02 ;FIC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0CF7105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0D4B105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DC0105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DC1105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DD6105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DDA105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DE9105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DEA105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DED105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DEE105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF2105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF6105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0DF7105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0E19105B&REV_02 ;FOXCONN
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11361734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11371734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11601734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_11611734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_118D1734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_118E1734&REV_02 ;FSC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_153410CF&REV_02 ;FUJI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_153510CF&REV_02 ;FUJI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_40021B0A&REV_02 ;HAIER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_40091B0A&REV_02 ;HAIER
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A85103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A88103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A8A103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A8C103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A97103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A98103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_2A9D103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3054103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3055103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3059103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3060103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3061103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3062103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3063103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3064103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3069103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_306A103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_306B103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_306C103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_306D103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30DE103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30F2103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30F3103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30F7103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30FB103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_30FE103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3600103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3602103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3603103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3607103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_360B103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3621103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3622103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3623103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3627103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3635103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3636103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3637103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3638103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3639103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363A103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363B103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363C103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363D103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363E103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_363F103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3642103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3643103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3644103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3649103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3650103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3652103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3656103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_3657103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_7010103C ;HP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00051170&REV_02 ;INVENTEC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_219D17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_389E17AA&REV_02 ;LENOVO
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17721854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17731854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17741854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17751854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17761854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17791854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17801854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17811854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17821854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17831854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17841854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17851854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17861854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17871854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17881854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17891854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_17901854&REV_02 ;LG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00021B7D&REV_02 ;MALATA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A0291071&REV_02 ;MITAC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_74001057&REV_02 ;MOTOROLA
;%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01101462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_100A1462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10171462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_101E1462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10271462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10281462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_102B1462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10311462&REV_02 ;MSI
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_88FA1033&REV_02 ;NEC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_890F1033&REV_02 ;NEC
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_018B1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_018C1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01931631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2141631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2151631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2181631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2191631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2161631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2171631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2181631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E2191631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_E21B1631&REV_02 ;PACKARDBELL
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_201F1B0A&REV_02 ;PEGATRON
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_1777152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0772152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0773152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0774152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0775152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0776152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0777152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0778152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0779152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0780152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0781152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0782152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0783152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0784152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0785152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0786152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0787152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0788152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_0789152D&REV_02 ;QUANTA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_B05F144D&REV_02 ;SAMSUNG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_B065144D&REV_02 ;SAMSUNG
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105713BD&REV_02 ;SHARP
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602A1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602B1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602C1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602D1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602E1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_602F1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60301509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60311509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60321509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60331509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60341509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60351509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60361509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60371509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60381509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_60391509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603A1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603B1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603C1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603D1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603E1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_603F1509&REV_02 ;STD
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00021179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_00031179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF1F1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF401179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF641179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF661179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF671179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF681179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FF6A1179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_FFC01179&REV_02 ;TOSHIBA
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003014C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003114C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003214C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003314C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003414C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003514C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003614C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003714C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003C14C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003D14C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_003E14C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_004614C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_004814C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_004914C0&REV_02 ;WB
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_A01414FF&REV_02 ;WHITE BOX
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_C2161631&REV_02 ;WISTRON
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_113A1734&REV_02 ;WISTRON
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_105317C0&REV_02 ;WISTRON
%RTL8102.DeviceDesc%	= RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_10C617C0&REV_02 ;WISTRON

;8401E
%RTL8401.DeviceDesc%    = RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&REV_04
%RTL8401.DeviceDesc%    = RTL8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_04

;8104E
%RTL8104.DeviceDesc%    = RTL8104a.ndi,     PCI\VEN_10EC&DEV_8137&REV_03
%RTL8104.DeviceDesc%    = RTL8104a.ndi,     PCI\VEN_10EC&DEV_8137&SUBSYS_813710EC&REV_03

;8168B
%RTL8168.DeviceDesc%  	= RTL8168a.ndi,	    PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%	= RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1077147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1078147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1079147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_107A147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_108D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C3C147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_240D147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2410147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2412147B&REV_01 ;ABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01071025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_010C1025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01261025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_26511025&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0B105B&REV_01 ;acer
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B1331897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B2201897&REV_01 ;AMTEK
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_060DA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0611A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0614A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0616A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061BA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_061CA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0623A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0624A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0625A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0631A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0634A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_063EA0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0636A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0640A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0642A0A0&REV_01 ;AOpen
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2055161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206A161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_206B161F&REV_01 ;Arima
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_11F51043&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81AA1043&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_53498086&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_D6068086&REV_01 ;ASUS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001940&REV_01 ;Channel
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05211558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05911558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_09021558&REV_01 ;Clevo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002014C0&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_002114C0&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;Compal
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_01 ;DELL
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_01 ;DELL
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F711019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F721019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F761019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F771019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F811019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0F821019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_902A1019&REV_01 ;ECS
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_90361695&REV_01 ;Epox
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_601F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60251509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_60291509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801A1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801C1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801D1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801E1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_801F1509&REV_01 ;FIC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C76105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7D105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C7E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C88105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C89105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C90105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C91105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0C92105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE6105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0CE7105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D0E105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1B105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D1C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D40105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D42105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D43105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D44105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D4C105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0D16105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE7105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DE9105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DEA105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DEE105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DEF105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF2105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DF9105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0DFD105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E17105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E18105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0E19105B&REV_01 ;Foxconn
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_111C1734&REV_01 ;FSC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_01 ;FSC(D45/D46)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0690107B&REV_01 ;GATEWAY
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0001458&REV_01 ;GBT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30B6103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_30CC103C&REV_01 ;HP Notebook
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_D6088086&REV_01 ;INTEL
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_00401170&REV_01 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_500E17FF&REV_01 ;Inventec
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_816816F3&REV_01 ;JETWAY
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_302917AA&REV_01 ;Lenovo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_303017AA&REV_01 ;Lenovo
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_01 ;LGE
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_47011071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_82521071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B3001071&REV_01 ;MiTAC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03411462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_03711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05311462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_05711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_238C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_270C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_276C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_279C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_280C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2F811462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FB31462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_2FBD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_309C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_327C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33201462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33371462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33411462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_334B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_337C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_338C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_33FF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_34131462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_345C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_348C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_356C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_367C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_368C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_369C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_373C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_375C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_376C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_379C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_384C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_387C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3F711462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB71462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FB91462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FCC1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FD51462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FDF1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FE91462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF31462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FF41462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_3FFE1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42CD1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42D71462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_42E11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43141462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43241462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_43271462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_514C1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63701462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63F21462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_63F41462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_65101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_65301462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_71901462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_71F11462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_72101462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_72301462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_73271462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732A1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_732B1462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80111854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80161854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_80171854&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4121462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A4221462&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E0151631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9011631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_E9021631&REV_01 ;MSI
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_83841033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_88071033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_887E1033&REV_01 ;NEC
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_20021B0A&REV_01 ;PEGATRON
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_058F17FF&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0761152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0762152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_0763152D&REV_01 ;RT_QTA
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B052144D&REV_01 ;SAMSUNG
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_B057144D&REV_01 ;SAMSUNG
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_104D13BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105013BD&REV_01 ;Sharp
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF001179&REV_01 ;Toshiba(Compal)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_FF011179&REV_01 ;Toshiba(Compal)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1091147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C41147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C43147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_1C46147B&REV_01 ;UABIT
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10CD1734&REV_01 ;Uniwill(FSC)
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_110E1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_105317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_10C317C0&REV_01 ;Wistron
%RTL8168.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_A00D14FF&REV_01 ;XPLORE
;8112
%RTL8112.DeviceDesc%    = RTL8168a.ndi,     PCI\VEN_10EC&DEV_8168&SUBSYS_83851043&REV_01

;8168C
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B2301897&REV_02 ;AMTEK
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01361025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_013E1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01401025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01441025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_014C1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_016D1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_016E1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02291025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02381025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_025F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02611025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_026F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027F1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02801025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02811025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02821025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02831025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02841025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02851025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02861025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02871025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02881025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02891025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_028A1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_028B1025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03021025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03031025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03041025&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_13601019&REV_02 ;ACER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_063AA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0643A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0644A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0646A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0648A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_064AA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_064EA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0700A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0703A0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_234EA0A0&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03E91AA7&REV_02 ;AOPEN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_16D51043&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_C2111631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_C2131631&REV_02 ;ASUS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080017FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080117FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080217FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080317FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080517FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_090017FF&REV_02 ;BENQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_302C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_313C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_398C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_501C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_513C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_519C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_528C1462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_73751462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75301462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75331462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75501462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75511462&REV_02 ;CHANNEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01261558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_03901558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04811558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_072F1558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08051558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08061558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_08601558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_09031558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_56011558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_70011558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76401558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76411558&REV_02 ;CLEVO
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_016B107B&REV_02 ;Compal
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_016D107B&REV_02 ;Compal
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02581028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02591028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_026F1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02731028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02751028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02781028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02791028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027D1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_027E1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02821028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02831028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02851028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02A91028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02AC1028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02B51028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02D91028&REV_02 ;DELL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_81111019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_81681019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90AD1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90AE1019&REV_02 ;ECS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50011509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50021509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50031509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50041509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_50051509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60421509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60431509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_80201509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_80211509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_80221509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_802C1509&REV_02 ;FIC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D0B105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D16105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D48105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D4C105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DDB105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DE3105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DE7105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DE9105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DEA105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DEE105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DEF105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF0105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DFD105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E0F105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E11105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E17105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E18105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E19105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E1C105B&REV_02 ;FOXCONN
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_11351734&REV_02 ;FSC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0900107B&REV_02 ;Gateway
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_1505103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_1506103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A6F103C&REV_02 ;HP cPC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A73103C&REV_02 ;HP bPC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A74103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A7F103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A80103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A82103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A85103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A88103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A8A103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2B00103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3038103C ;HP-CDC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_303A103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_303B103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3043103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3045103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30DE103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F1103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F2103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F4103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F7103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30F8103C ;HPQ
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30FB103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_30FC103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3600103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3602103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3603103C&REV_02 ;HP Notebook
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_360F103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3610103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_361B103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_361C103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_361D103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_361E103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3621103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3622103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3624103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3628103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3629103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3633103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_7010103C ;HP
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_000E1B0A&REV_02 ;HAIER
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_001F1B0A&REV_02 ;HAIER(EPSON)
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6098086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6128086&REV_02 ;INTEL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01171854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01181854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01191854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_011A1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_011F1854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01201854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01211854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01221854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17721854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17731854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17741854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17751854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17761854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17791854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17801854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17881854&REV_02 ;LGE
;%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17891854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_20021854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_20031854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_20071854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10051462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10081462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10181462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_22701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_392C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_43201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_43501462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_43701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_43801462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_515C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_520C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_522C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_536C1462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_63F51462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_65101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_65201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_67401462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_71F01462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_72201462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_73881462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75121462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75161462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75221462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75261462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75321462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75351462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75431462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75461462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75491462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75521462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75581462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75641462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75661462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75691462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75701462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75721462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75931462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A1101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_83691033&REV_02 ;NEC
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00031B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_006A1B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_200B1B0A&REV_02 ;PEGATRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0772152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0773152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0774152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0775152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0776152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0777152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0779152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0780152D&REV_02 ;QUANTA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B04E144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B052144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B057144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_B063144D&REV_02 ;SAMSUNG
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00201B0A&REV_02 ;SI
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602A1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602B1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602C1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602D1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602E1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_602F1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60301509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60311509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60321509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60331509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60341509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60351509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60361509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60371509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60381509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60391509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603A1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603B1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603C1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603D1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603E1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_603F1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60401509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60411509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60421509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60431509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60441509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60451509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60461509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60471509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60481509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60491509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604A1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604B1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604C1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604D1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604E1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_604F1509&REV_02 ;STD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_82E919DB&REV_02 ;TCL
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_210817AA&REV_02 ;THINKPAD
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00091290&REV_02 ;TOPS
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_60341991&REV_02 ;TOPSTAR
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00011179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1C1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1E1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1F1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF601179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF621179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF671179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF7A1179&REV_02 ;TOSHIBA
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_109C147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_1102147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_1103147B&REV_02 ;UABIT
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003014C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003114C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003214C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003314C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003414C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003514C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003614C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003714C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003914C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003C14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003D14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_003E14C0&REV_02 ;WB
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A00C14FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A01514FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A01614FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_A02014FF&REV_02 ;WHITE BOX
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113B1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113D1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113E1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_11631734&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10C017C0&REV_02 ;WISTRON
%RTL8168C.DeviceDesc%   = RTL8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_409017C0&REV_02 ;WISTRON
;8168CASUS
%RTL8168C.DeviceDesc%   = RTL8168CASUSa.ndi,PCI\VEN_10EC&DEV_8168&SUBSYS_82FF1043&REV_02 ;ASUS
;8168CForceGigabit
%RTL8168C.DeviceDesc%   = RTL8168CForceGigabita.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_83AB1043&REV_02 ;ASUS
;8168CMitac
%RTL8168C.DeviceDesc%   = RTL8168CMitaca.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_92131071&REV_02 ;Mitac

;8168D
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&REV_03
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_03
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_024E1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_024F1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_025A1025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02661025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02761025&REV_03 ;ACER
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0700A0A0&REV_03 ;AOPEN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_16D51043&REV_03 ;ASUS
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_080417FF&REV_03 ;BENQ
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_01301558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_86871558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_86891558&REV_03 ;CLEVO
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02BA1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02BB1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02BC1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02BD1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02C01028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02D81028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02EA1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02EB1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02F21028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_02F51028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04011028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04021028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04031028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04081028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04151028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04161028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_04181028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_041E1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_041F1028&REV_03 ;DELL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_811D1019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_8D481019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90931019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90B61019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_90B71019&REV_03 ;ECS
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_400A1B0A&REV_03 ;
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0D41105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DC0105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DC1105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DD4105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DDA105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DED105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF2105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF6105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0DF7105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E0C105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0E0D105B&REV_03 ;FOXCONN
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_113F1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_118D1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_118E1734&REV_03 ;FSC
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0256103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A8E103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A90103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A92103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A94103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A97103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_2A9C103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3046103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3059103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3060103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3061103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3062103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3063103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3064103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_306D103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3635103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3636103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3637103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3638103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3639103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363B103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363C103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363D103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363E103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_363F103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_3652103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_7001103C ;HP
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00671170&REV_03 ;INVENTEC
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6138086&REV_03 ;INTEL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_D6148086&REV_03 ;INTEL
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_210817AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_213117AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_306917AA&REV_03 ;LENOVO
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_38A017AA&REV_03 ;LENOVO
;%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17811854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17821854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17831854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17841854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17851854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17861854&REV_03 ;LG
;%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17871854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_92231071&REV_03 ;MITAC
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_92701071&REV_03 ;MITAC
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_74001057&REV_03 ;MOTOROLA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10041462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10061462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10081462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_100E1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_100F1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10111462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10121462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_101C1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_101D1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_101F1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10201462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10211462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10221462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_102D1462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75261462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75631462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75741462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75761462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75771462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75791462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75801462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75811462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75861462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75871462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75921462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75951462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75961462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_75991462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76021462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_76091462&REV_03 ;MSI
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_12021849&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_15011849&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_20221B0A&REV_03 ;PEGATRON
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0784152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0785152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0786152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0787152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0788152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_0789152D&REV_03 ;QUANTA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_00021179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1E1179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF1F1179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FF401179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_FFC01179&REV_03 ;TOSHIBA
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_004614C0&REV_03 ;WB
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_004814C0&REV_03 ;WB
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_004914C0&REV_03 ;WB
%RTL8168D.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_10CB17C0&REV_03 ;WISTRON


;8112L
%RTL8112L.DeviceDesc%   = RTL8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_83A31043&REV_03

; 8168DP
%RTL8168DP.DeviceDesc%  = RTL8168DPa.ndi,   PCI\VEN_10EC&DEV_8168&REV_04
%RTL8168DP.DeviceDesc%  = RTL8168DPa.ndi,   PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_04

;PNP_CHG_XP64
%RTL8102.DeviceDesc%	= RTLChgPnpCaps8102a.ndi,     PCI\VEN_10EC&DEV_8136&SUBSYS_01101462&REV_02 ;MSI
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17721854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17731854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17741854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17751854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17761854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17791854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17801854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17881854&REV_02 ;LGE
%RTL8168C.DeviceDesc%   = RTLChgPnpCaps8168Ca.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17891854&REV_02 ;LGE
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17811854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17821854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17831854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17841854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17851854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17861854&REV_03 ;LG
%RTL8168D.DeviceDesc%   = RTLChgPnpCaps8168Da.ndi,    PCI\VEN_10EC&DEV_8168&SUBSYS_17871854&REV_03 ;LG

;;****************************************************************************
;; Windows 98/ME
;;****************************************************************************
;;RTL8168(98/ME)
[RTL8168.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168C(98/ME)
[RTL8168C.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168C ASUS(98/ME)
[RTL8168CASUS.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = WolCap.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168C ForceGigabit(98/ME)
[RTL8168CForceGigabit.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed1g.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolS5LinkSpeedForce1g.reg
AddReg          = WolCap.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168C Mitac(98/ME)
[RTL8168CMitac.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = WolCap.reg, ForceMode.reg, GreenEthernetDisabled.reg,RxDescNumber.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168D(98/ME)
[RTL8168D.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8168DP(98/ME)
[RTL8168DP.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8168.id.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8136(98/ME)
[RTL8136.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8136 HP(98/ME)
[RTL8136HP.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = AutoCrossoverDet.reg, WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8102E(98/ME)
[RTL8102.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

;;****************************************************************************
;;RTL8104E(98/ME)
[RTL8104.ndi]
DriverVer       = 06/04/2009,728
AddReg          = rtl8136.id.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = WolCap.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles9x

[Rtlnic.CopyFiles9x]
Rtenic.sys,,,2

;;****************************************************************************
;; Windows 2000
;;****************************************************************************
;;RTL8168(W2K)
[RTL8168.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(W2K)
[RTL8168C.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168C.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ASUS(W2K)
[RTL8168CASUS.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168CASUS.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;RTL8168C ForceGigabit(W2K)
[RTL8168CForceGigabit.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed1g.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolS5LinkSpeedForce1g.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168CForceGigabit.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168CMitac(W2K)
[RTL8168CMitac.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg,RxDescNumber.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168CMitac.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168D(W2K)
[RTL8168D.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168D.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8168DP(W2K)
[RTL8168DP.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8168DP.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8136(W2K)
[RTL8136.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8136.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8136 HP(W2K)
[RTL8136HP.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8136HP.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(W2K)
[RTL8102.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8102.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

;;****************************************************************************
;;RTL8104E(W2K)
[RTL8104.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFiles, RTNicProp.CopyList2K

[RTL8104.ndi.NT.Services]
AddService      = RTLE8023, 2, rtsnt.Service, common.EventLog

[Rtlnic.CopyFiles]
Rtenic.sys,,,2

[RTNicProp.CopyList2K]
RtNicProp32.dll,,,0x02

;;****************************************************************************
;; Windows XP
;;****************************************************************************
;;RTL8168(XP)
[RTL8168x.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(XP)
[RTL8168Cx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168Cx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ASUS(XP)
[RTL8168CASUSx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168CASUSx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ForceGigabit(XP)
[RTL8168CForceGigabitx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed1g.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolS5LinkSpeedForce1g.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168CForceGigabitx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C Mitac(XP)
[RTL8168CMitacx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg,RxDescNumber.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168CMitacx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(XP)
[RTLChgPnpCaps8168Cx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetDisabled.reg, ChgPnp.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTLChgPnpCaps8168Cx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168D(XP)
[RTL8168Dx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168Dx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168DP(XP)
[RTL8168DPx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8168DPx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8168D(XP)
[RTLChgPnpCaps8168Dx.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, GreenEthernetEnabled.reg,  ChgPnp.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTLChgPnpCaps8168Dx.ndi.NT.Services]
AddService = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8136(XP)
[RTL8136x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8136x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8136HP(XP)
[RTL8136HPx.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8136HPx.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(XP)
[RTL8102x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8102x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog


;;****************************************************************************
;;RTL8102E(XP)
[RTLChgPnpCaps8102x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg, ChgPnp.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTLChgPnpCaps8102x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

;;****************************************************************************
;;RTL8104E(XP)
[RTL8104x.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023xp.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp32.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesXP, RTNicProp.CopyListXP

[RTL8104x.ndi.NT.Services]
AddService      = RTLE8023xp, 2, rtsntxp.Service, common.EventLog

[Rtlnic.CopyFilesXP]
Rtenicxp.sys,,,2

[RTNicProp.CopyListXP]
RtNicProp32.dll,,,0x02

;;****************************************************************************
;; Windows XP 64-bit
;;****************************************************************************
;;RTL8168(XP64)
[RTL8168a.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68BJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C(XP64)
[RTL8168Ca.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168Ca.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ASUS(XP64)
[RTL8168CASUSa.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168CASUSa.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C ForceGigabit(XP64)
[RTL8168CForceGigabita.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed1g.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolS5LinkSpeedForce1g.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetDisabled.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168CForceGigabita.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C Mitac(XP64)
[RTL8168CMitaca.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeedIntel.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetDisabled.reg,RxDescNumber.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168CMitaca.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168C (XP64)
[RTLChgPnpCaps8168Ca.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg 
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetDisabled.reg, ChgPnp.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTLChgPnpCaps8168Ca.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168D(XP64)
[RTL8168Da.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168Da.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168DP(XP64)
[RTL8168DPa.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetEnabled.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8168DPa.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8168D(XP64)
[RTLChgPnpCaps8168Da.ndi.NT]
DelReg          = GigPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed.reg, 68CJumboframe.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg, GreenEthernetEnabled.reg, ChgPnp.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTLChgPnpCaps8168Da.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8136(XP64)
[RTL8136a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8136a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8136 HP(XP64)
[RTL8136HPa.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, AutoCrossoverDet.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8136HPa.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(XP64)
[RTL8102a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8102a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8102E(XP64)
[RTLChgPnpCaps8102a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg, ChgPnp.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTLChgPnpCaps8102a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

;;****************************************************************************
;;RTL8104E(XP64)
[RTL8104a.ndi.NT]
DelReg          = TsPreParams.DelReg
Characteristics = 0x84
BusType         = 5
AddReg          = RTLE8023x64.reg, NetworkAddress.reg, Speed10_100.reg, Flowctrl.reg, S5Wol.reg, WolShutdownLinkSpeed.reg
AddReg          = OffloadChksum.reg, OffloadLargesend.reg, VLanTagging.reg, WolCap.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = RtNicProp64.reg, ForceMode.reg
CopyFiles       = Rtlnic.CopyFilesX64, RTNicProp.CopyListX64

[RTL8104a.ndi.NT.Services]
AddService      = RTLE8023x64, 2, rtsntx64.Service, common.EventLog

[Rtlnic.CopyFilesX64]
Rtenic64.sys,,,2

[RTNicProp.CopyListX64]
RtNicProp64.dll,,,0x02

;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[rtl8168.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtenic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTLE8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8168"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

[rtl8136.id.reg]
HKR,,               MediaType,        0, 1
HKR,,               AdapterType,      0, 5
HKR,,               BusType,          0, 5
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "Rtenic.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,NDIS,           LogDriverName,    0, "RTLE8023"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            DeviceID,         0, "PCI\VEN_10EC&DEV_8136"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"  
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;;****************************************************************************
;; Del parameters
;;****************************************************************************
[GigPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\WakeOnLanSpeed
HKR,,WakeOnLanSpeed
;HKR,Ndi\Params\S5WakeOnLan
;HKR,,S5WakeOnLan
HKR,,SuperSwitch
HKR,,PowerDownPll

[TsPreParams.DelReg]
HKR,Ndi\Params\WakeUpFrame
HKR,,WakeUpFrame
HKR,Ndi\Params\NumTxDesc
HKR,,NumTxDesc
HKR,Ndi\Params\NumRxDesc
HKR,,NumRxDesc
HKR,Ndi\Params\NumTxDescHPQ
HKR,,NumTxDescHPQ
HKR,Ndi\Params\RegVlanid
HKR,,RegVlanid
HKR,Ndi\Params\WakeOnLanSpeed
HKR,,WakeOnLanSpeed
;HKR,Ndi\Params\S5WakeOnLan
;HKR,,S5WakeOnLan

;;****************************************************************************
;; common parameters
;;****************************************************************************

[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	type,		0, "edit"
HKR,Ndi\params\NetworkAddress,	default,	0, "000000000000"
HKR,Ndi\params\NetworkAddress,	LimitText,	0, "12"
HKR,Ndi\params\NetworkAddress,	UpperCase,	0, "1"
HKR,Ndi\params\NetworkAddress,	Optional,	0, "1"

[Speed.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR, Ndi\params\DuplexMode\enum,  6,          0, %sd1000full%
HKR,,DuplexMode,0,"1"

[Speed10_100.reg]
HKR, Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR, Ndi\params\DuplexMode,       type,       0, "enum"
HKR, Ndi\params\DuplexMode,       default,    0, "1"
HKR, Ndi\params\DuplexMode\enum,  1,          0, %auto_nego%
HKR, Ndi\params\DuplexMode\enum,  2,          0, %sd10half%
HKR, Ndi\params\DuplexMode\enum,  3,          0, %sd10full%
HKR, Ndi\params\DuplexMode\enum,  4,          0, %sd100half%
HKR, Ndi\params\DuplexMode\enum,  5,          0, %sd100full%
HKR,,DuplexMode,0,"1"

[Speed1g.reg]
HKR,Ndi\params\DuplexMode,       ParamDesc,  0, %SpeedDuplexMode%
HKR,Ndi\params\DuplexMode,       default,    0, "6"
HKR,Ndi\params\DuplexMode,       type,       0, "enum"
HKR,Ndi\params\DuplexMode\enum,  "6",        0, %sd1000full%
HKR,,*SpeedDuplex,0,"6"

;[TxDescNumber.reg]
;HKR,Ndi\Params\NumTxDesc,         ParamDesc,  0, %TxDescNumber%
;HKR,Ndi\Params\NumTxDesc,         Type,       0, "int"
;HKR,Ndi\Params\NumTxDesc,         Default,    0, "256"
;HKR,Ndi\Params\NumTxDesc,         Min,        0, "64"
;HKR,Ndi\Params\NumTxDesc,         Max,        0, "512"
;HKR,Ndi\Params\NumTxDesc,         Step,       0, "1"
;HKR,Ndi\Params\NumTxDesc,         Base,       0, "10"
;HKR,,NumTxDesc,0,"256"

[RxDescNumber.reg]
HKR,Ndi\Params\NumRxDesc,         ParamDesc,  0, %RxDescNumber%
HKR,Ndi\Params\NumRxDesc,         Type,       0, "int"
HKR,Ndi\Params\NumRxDesc,         Default,    0, "512"
HKR,Ndi\Params\NumRxDesc,         Min,        0, "256"
HKR,Ndi\Params\NumRxDesc,         Max,        0, "1024"
HKR,Ndi\Params\NumRxDesc,         Step,       0, "1"
HKR,Ndi\Params\NumRxDesc,         Base,       0, "10"
HKR,,NumRxDesc,0,"512"

[68BJumboframe.reg]
HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, %Disabled%
HKR,Ndi\params\Jumboframe\enum,   "1",        0, %2KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "2",        0, %3KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "3",        0, %4KBMTU%
HKR,,Jumboframe,0,"0"

[68CJumboframe.reg]
HKR,Ndi\params\Jumboframe,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\Jumboframe,        default,    0, "0"
HKR,Ndi\params\Jumboframe,        type,       0, "enum"
HKR,Ndi\params\Jumboframe\enum,   "0",        0, %Disabled%
HKR,Ndi\params\Jumboframe\enum,   "1",        0, %2KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "2",        0, %3KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "3",        0, %4KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "4",        0, %5KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "5",        0, %6KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "6",        0, %7KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "7",        0, %8KBMTU%
HKR,Ndi\params\Jumboframe\enum,   "8",        0, %9KBMTU%
HKR,,Jumboframe,0,"0"

[Flowctrl.reg]
HKR,Ndi\params\FlowControl,      ParamDesc,  0, %FlowControl%
HKR,Ndi\params\FlowControl,      default,    0, "1"
HKR,Ndi\params\FlowControl,      type,       0, "enum"
HKR,Ndi\params\FlowControl\enum, "0",        0, %Disabled%
HKR,Ndi\params\FlowControl\enum, "1",        0, %Enabled%
HKR,,FlowControl,0,"1" 

[S5Wol.reg]
HKR,Ndi\params\S5WakeOnLan,      ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,      default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,      type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum, "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum, "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[powersavingautophy.reg]
HKR,Ndi\params\AutoLinkDownPhyOff,       ParamDesc,  0, %AutoLinkDownPhyOff%
HKR,Ndi\params\AutoLinkDownPhyOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPhyOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPhyOff,0,"0"

[powersavingautopcie.reg]
HKR,Ndi\params\AutoLinkDownPcieMacOff,       ParamDesc,  0, %AutoLinkDownPcieMacOff%
HKR,Ndi\params\AutoLinkDownPcieMacOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPcieMacOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPcieMacOff,0,"0"

[WolShutdownLinkSpeed.reg]
HKR, Ndi\params\WolShutdownLinkSpeed,       ParamDesc,  0, %WolShutdownLinkSpeed%
HKR, Ndi\params\WolShutdownLinkSpeed,       type,       0, "enum"
HKR, Ndi\params\WolShutdownLinkSpeed,       default,    0, "0"
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "0",        0, %10MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "1",        0, %100MbFirst%
HKR,,WolShutdownLinkSpeed,0,"0"

[WolShutdownLinkSpeedIntel.reg]
HKR, Ndi\params\WolShutdownLinkSpeed,       ParamDesc,  0, %WolShutdownLinkSpeed%
HKR, Ndi\params\WolShutdownLinkSpeed,       type,       0, "enum"
HKR, Ndi\params\WolShutdownLinkSpeed,       default,    0, "2"
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "0",        0, %10MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "1",        0, %100MbFirst%
HKR, Ndi\params\WolShutdownLinkSpeed\enum,  "2",        0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolS5LinkSpeedForce1g.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,	    ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,	    default,    0, "2"
HKR,Ndi\params\WolShutdownLinkSpeed,        type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolCap.reg]
HKR, Ndi\params\WolCap,            ParamDesc,  0, %WolCap%
HKR, Ndi\params\WolCap,            type,       0, "enum"
HKR, Ndi\params\WolCap,            default,    0, "3"
HKR, Ndi\params\WolCap\enum,       "0",        0, %None%
HKR, Ndi\params\WolCap\enum,       "1",        0, %PatternMatch%
HKR, Ndi\params\WolCap\enum,       "2",        0, %MagicPacket%
HKR, Ndi\params\WolCap\enum,       "3",        0, %PatternAndMagic%
HKR,,WolCap,0,"3"

[GreenEthernetEnabled.reg]
HKR,Ndi\params\GreenEthernet,      ParamDesc,  0, %GreenEthernet%
HKR,Ndi\params\GreenEthernet,      default,    0, "1"
HKR,Ndi\params\GreenEthernet,      type,       0, "enum"
HKR,Ndi\params\GreenEthernet\enum, "0",        0, %Disabled%
HKR,Ndi\params\GreenEthernet\enum, "1",        0, %Enabled%
HKR,,GreenEthernet,0,"1"

[GreenEthernetDisabled.reg]
HKR,Ndi\params\GreenEthernet,      ParamDesc,  0, %GreenEthernet%
HKR,Ndi\params\GreenEthernet,      default,    0, "0"
HKR,Ndi\params\GreenEthernet,      type,       0, "enum"
HKR,Ndi\params\GreenEthernet\enum, "0",        0, %Disabled%
HKR,Ndi\params\GreenEthernet\enum, "1",        0, %Enabled%
HKR,,GreenEthernet,0,"0"

;[AutoSpeedDown.reg]
;HKR,Ndi\params\AutoSpeedDown,         ParamDesc,  0, %AutoSpeedDown%
;HKR,Ndi\params\AutoSpeedDown,         default,    0, "1"
;HKR,Ndi\params\AutoSpeedDown,         type,       0, "enum"
;HKR,Ndi\params\AutoSpeedDown\enum,    "0",        0, %Disabled%
;HKR,Ndi\params\AutoSpeedDown\enum,    "1",        0, %Enabled%
;HKR,,AutoSpeedDown,0,"1"

;[SuperSwitch.reg]
;HKR,,SuperSwitch,0,"0"

[PowerDownPll.reg]
HKR,,PowerDownPll,0,"0"

[ForceMode.reg]
HKR,,ForceMode,0,"0"

[ChgPnp.reg]
HKR,,PnPCapabilities,0x10001,0x0020

[RtNicProp32.reg]
HKR,,EnumPropPages32,,"rtnicprop32.dll,RTNicPropPageProvider"

[RtNicProp64.reg]
HKR,,EnumPropPages32,,"rtnicprop64.dll,RTNicPropPageProvider"

;;****************************************************************************
;; NT parameters
;;****************************************************************************

[OffloadChksum.reg]
HKR,Ndi\params\CksOffload,        ParamDesc,  0, %ChecksumOffload%
HKR,Ndi\params\CksOffload,        default,    0, "1"
HKR,Ndi\params\CksOffload,        type,       0, "enum"
HKR,Ndi\params\CksOffload\enum,   "0",        0, %Disabled%
HKR,Ndi\params\CksOffload\enum,   "1",        0, %RxTxEnabled%
HKR,Ndi\params\CksOffload\enum,   "3",        0, %RxEnabled%
HKR,Ndi\params\CksOffload\enum,   "4",        0, %TxEnabled%
HKR,,CksOffload,0,"1" 

[OffloadLargesend.reg]
HKR,Ndi\params\Largesend,         ParamDesc,  0, %LargesendOffload%
HKR,Ndi\params\Largesend,         default,    0, "1"
HKR,Ndi\params\Largesend,         type,       0, "enum"
HKR,Ndi\params\Largesend\enum,    "0",        0, %Disabled%
HKR,Ndi\params\Largesend\enum,    "1",        0, %Enabled%
HKR,,Largesend,0,"1" 

[VLanTagging.reg]
HKR,Ndi\params\Support8021p,      ParamDesc,  0, %VLanTagging%
HKR,Ndi\params\Support8021p,      default,    0, "0"
HKR,Ndi\params\Support8021p,      type,       0, "enum"
HKR,Ndi\params\Support8021p\enum, "0",        0, %Disabled%
HKR,Ndi\params\Support8021p\enum, "1",        0, %Enabled%
HKR,,Support8021p,0,"0" 

;[VLanID.reg]
;HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
;HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
;HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
;HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
;HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
;HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
;HKR,Ndi\Params\RegVlanid,   Base,       0, "10"
;HKR,,RegVlanid,0,"0" 

;[TxHPQDescNumber.reg]
;HKR,Ndi\Params\NumTxDescHPQ,      ParamDesc,  0, %TxHPQDescNumber%
;HKR,Ndi\Params\NumTxDescHPQ,      Type,       0, "int"
;HKR,Ndi\Params\NumTxDescHPQ,      Default,    0, "256"
;HKR,Ndi\Params\NumTxDescHPQ,      Min,        0, "64"
;HKR,Ndi\Params\NumTxDescHPQ,      Max,        0, "512"
;HKR,Ndi\Params\NumTxDescHPQ,      Step,       0, "1"
;HKR,Ndi\Params\NumTxDescHPQ,      Base,       0, "10"
;HKR,,NumTxDescHPQ,0,"256" 

[AutoCrossoverDet.reg]
HKR,Ndi\params\AutoCrossoverDet,	ParamDesc,  0, %AutoCrossoverDet%
HKR,Ndi\params\AutoCrossoverDet,	default,    0, "0"
HKR,Ndi\params\AutoCrossoverDet,	type,       0, "enum"
HKR,Ndi\params\AutoCrossoverDet\enum,   "0",        0, %Disabled%
HKR,Ndi\params\AutoCrossoverDet\enum,   "1",        0, %Enabled%
HKR,,AutoCrossoverDet,0,"0"

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTLE8023.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023"

[rtsnt.Service]
DisplayName     = %Rtlnic.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenic.sys
LoadOrderGroup  = NDIS

[RTLE8023xp.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023xp"

[rtsntxp.Service]
DisplayName     = %Rtlnicxp.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenicxp.sys
LoadOrderGroup  = NDIS

[RTLE8023x64.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTLE8023x64"

[rtsntx64.Service]
DisplayName     = %Rtlnicx64.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtenic64.sys
LoadOrderGroup  = NDIS

[common.EventLog]
Addreg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
Rtlnic.CopyFiles           = 12
Rtlnic.CopyFilesXP         = 12
Rtlnic.CopyFilesX64        = 12
Rtlnic.CopyFiles9x         = 11
RTNicProp.CopyList2k       = 11
RTNicProp.CopyListXP       = 11
RTNicProp.CopyListX64      = 11
DefaultDestDir             = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
Rtenic.sys	= 1
Rtenicxp.sys	= 1
Rtenic64.sys	= 1
RTNicProp32.dll	= 1
RTNicProp64.dll	= 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p VLAN Tagging"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Checksum Offload"
LargesendOffload	= "Large Send Offload"
SpeedDuplexMode		= "Speed & Duplex"
auto_nego		= "Auto Negotiation"
sd10half		= "10 Mbps Half Duplex"
sd10full		= "10 Mbps Full Duplex"
sd100half		= "100 Mbps Half Duplex"
sd100full		= "100 Mbps Full Duplex"
sd1000full		= "1.0 Gbps Full Duplex"
NetworkAddress		= "Network Address"
JumboFrame		= "Jumbo Frame"
;TxDescNumber		= "Number of Tx Descriptor"
RxDescNumber		= "Number of Rx Descriptor"
;TxHPQDescNumber	= "Number of High Priority Tx Descriptor"
FlowControl		= "Flow Control"
;AutoSpeedDown		= "Auto Speed Down"
S5WakeOnLan		= "Shutdown Wake-On-Lan"
10MbFirst               = "10 Mbps First"
100MbFirst              = "100 Mbps First"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "WOL & Shutdown Link Speed"
AutoCrossoverDet        = "Auto Crossover Detection"
Disabled                = "Disabled"
Enabled                 = "Enabled"
TxEnabled               = "Tx Enabled"
RxEnabled               = "Rx Enabled"
RxTxEnabled             = "Rx & Tx Enabled"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "Auto Disable PCIe (PowerSaving)"
AutoLinkDownPhyOff      = "Auto Disable PHY (PowerSaving)"
Battery                 = "Enabled, Battery"
AcBattery               = "Enabled, Battery or AC"
GreenEthernet           = "Green Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Arabic_UAE
[Strings.3801]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "تحديد شبكة اتصال محلية افتراضية 802.1Q/1p"
;VLanID			= "معرف شبكة اتصال محلية افتراضية 802.1Q"
ChecksumOffload		= "تحميل المجموع الاختباري"
LargesendOffload	= "تحميل الإرسال الكبير"
SpeedDuplexMode		= "السرعة والازدواج"
auto_nego		= "التفاوض التلقائي"
sd10half		= "نصف المزدوج 10 ميجا بايت في الثانية"
sd10full		= "كامل الازدواج 10 ميجا بايت في الثانية"
sd100half		= "كامل الازدواج 100 ميجا بايت في الثانية"
sd100full		= "كامل الازدواج 100 ميجا بايت في الثانية"
sd1000full		= "كامل الازدواج 1000 ميجا بايت في الثانية"
NetworkAddress		= "عنوان الشبكة"
JumboFrame		= "الإطار الضخم"
;TxDescNumber		= "رقم واصف النقل"
RxDescNumber		= "رقم واصف الاستقبال"
;TxHPQDescNumber	= "رقم واصف النقل ذي الأولوية القصوى"
FlowControl		= "التحكم بالانسياب"
;AutoSpeedDown		= "خفض السرعة التلقائية"
S5WakeOnLan		= "إغلاق معيار Wake-On-Lan"
10MbFirst               = "10 ميجا بايت في الثانية أولا"
100MbFirst              = "100 ميجا بايت في الثانية أولا"
NotSpeedDown            = "عدم تخفيض السرعة"
WolShutdownLinkSpeed    = "رابط السرعة للإغلاق ومعيار Wake-On-Lan"
AutoCrossoverDet        = "رصد التحويل التلقائي"
Disabled                = "تعطيل"
Enabled                 = "تمكين"
TxEnabled               = "Tx قيد التمكين"
RxEnabled               = "Rx قيد التمكين"
RxTxEnabled             = "Rx & Tx قيد التمكين"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "قدرات تنشيط Lan"
None                    = "لا شيء"
PatternMatch            = "مطابقة عامل البحث"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "مطابقة عامل البحث وMagic Packet"
AutoLinkDownPcieMacOff  ="تعطيل تلقائي PowerSaving) PCIe)"
AutoLinkDownPhyOff      ="تعطيل تلقائي PowerSaving) PHY)"
Battery                 = "قيد التمكين، البطارية"
AcBattery               ="قيد التمكين، البطارية أو التيار المتردد"
GreenEthernet           = "إيثرنت أخضر"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Chinese_Taiwan
[Strings.0404]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p 虛擬網路標籤"
;VLanID			= "802.1Q 虛擬網路識別碼"
ChecksumOffload		= "檢查總和值卸載"
LargesendOffload	= "大量傳送卸載"
SpeedDuplexMode		= "連線速度和雙工模式"
auto_nego		= "自動偵測"
sd10half		= "10 Mbps 半雙工"
sd10full		= "10 Mbps 全雙工"
sd100half		= "100 Mbps 半雙工"
sd100full		= "100 Mbps 全雙工"
sd1000full		= "1.0 Gbps 全雙工"
NetworkAddress		= "網路卡位址"
JumboFrame		= "巨大訊框"
;TxDescNumber		= "傳送端描述子數目"
RxDescNumber		= "接收端描述子數目"
;TxHPQDescNumber	= "高優先權傳送端描述子數目"
FlowControl		= "流量控制"
;AutoSpeedDown		= "自動降速"
S5WakeOnLan		= "關機網路喚醒"
10MbFirst               = "10 Mbps 優先"
100MbFirst              = "100 Mbps 優先"
NotSpeedDown            = "不要降速"
WolShutdownLinkSpeed    = "網路喚醒和關機連線速度"
AutoCrossoverDet        = "自動跳線偵測"
Disabled                = "關閉"
Enabled                 = "開啟"
TxEnabled               = "Tx 開啟"
RxEnabled               = "Rx 開啟"
RxTxEnabled             = "Rx & Tx 開啟"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "網路喚醒模式"
None                    = "無"
PatternMatch            = "樣式比對"
MagicPacket             = "魔術封包"
PatternAndMagic         = "樣式比對及魔術封包"
AutoLinkDownPcieMacOff  = "自動關閉 PCIe (省電)"
AutoLinkDownPhyOff      = "自動關閉 PHY (省電)"
Battery                 = "開啟, 電池"
AcBattery               = "開啟, 電池或 AC"
GreenEthernet           = "環保節能"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Chinese_PRC
[Strings.0804]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p 虚拟网路标签"
;VLanID			= "802.1Q 虚拟网路识别码"
ChecksumOffload		= "硬件校验和"
LargesendOffload	= "大量传送减负"
SpeedDuplexMode		= "连接速度和双工模式"
auto_nego		= "自动侦测"
sd10half		= "10 Mbps 半双工"
sd10full		= "10 Mbps 全双工"
sd100half		= "100 Mbps 半双工"
sd100full		= "100 Mbps 全双工"
sd1000full		= "1.0 Gbps 全双工"
NetworkAddress		= "网路卡位址"
JumboFrame		= "巨型帧"
;TxDescNumber		= "传送端描述符数目"
RxDescNumber		= "接收端描述符数目"
;TxHPQDescNumber	= "高优先权传送端描述符数目"
FlowControl		= "流控制"
;AutoSpeedDown		= "自动降速"
S5WakeOnLan             = "关机 网络唤醒"
10MbFirst               = "10 Mbps 优先"
100MbFirst              = "100 Mbps 优先"
NotSpeedDown            = "不要降速"
WolShutdownLinkSpeed    = "网络唤醒和关机连接速度"
AutoCrossoverDet        = "自动跳线侦测"
Disabled                = "关闭"
Enabled                 = "开启"
TxEnabled               = "Tx 开启"
RxEnabled               = "Rx 开启"
RxTxEnabled             = "Rx & Tx 开启"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "网路唤醒模式"
None                    = "无"
PatternMatch            = "样式比对"
MagicPacket             = "魔术封包"
PatternAndMagic         = "样式比对及魔术封包"
AutoLinkDownPcieMacOff  = "自动关闭 PCIe (省电)"
AutoLinkDownPhyOff      = "自动关闭 PHY (省电)"
Battery                 = "开启, 电池"
AcBattery               = "开启, 电池或者交流电源"
GreenEthernet           = "环保节能"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Czech
[Strings.0405]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging	        = "Značkování paketů VLAN 802.1Q/1p"
;VLanID	                = "ID VLAN 802.1Q"
ChecksumOffload	        = "Výpočet kontrolních součtů"
LargesendOffload	= "Zpracování velkých segmentů (LSO)"
SpeedDuplexMode	        = "Rychlost a přenosový režim"
auto_nego	        = "Automatické nastavení režimu provozu"
sd10half       	        = "Poloduplexní 10 Mbps"
sd10full	        = "Plně duplexní 10 Mbps"
sd100half	        = "Poloduplexní 100 Mbps"
sd100full	        = "Plně duplexní 100 Mbps"
sd1000full	        = "Plně duplexní 1,0 Gbps"
NetworkAddress	        = "Síťová adresa"
JumboFrame	        = "Jumbo rámec"
;TxDescNumber	        = "Číslo deskriptoru odesílání"
RxDescNumber	        = "Číslo deskriptoru příjmu"
;TxHPQDescNumber	= "Číslo deskriptoru odesílání s vysokou prioritou"
FlowControl	        = "Řízení toku"
;AutoSpeedDown	        = "Automatické zpomalení"
S5WakeOnLan	        = "Zapnutí vypnutého počítače přes síť"
10MbFirst	        = "Nejdříve 10 Mbps"
100MbFirst	        = "Nejdříve 100 Mbps"
NotSpeedDown	        = "Bez zpomalení"
WolShutdownLinkSpeed	= "Rychlost linky pro WOL a vypnutí"
AutoCrossoverDet	= "Automatická detekce křížených kabelů"
Disabled	        = "Zakázáno"
Enabled	                = "Povoleno"
TxEnabled	        = "Odesílání povoleno"
RxEnabled	        = "Příjem povolen"
RxTxEnabled	        = "Příjem a odesílání povoleno"
2KBMTU	                = "2 KB MTU"
3KBMTU	                = "3 KB MTU"
4KBMTU	                = "4 KB MTU"
5KBMTU	                = "5 KB MTU"
6KBMTU              	= "6 KB MTU"
7KBMTU	                = "7 KB MTU"
8KBMTU	                = "8 KB MTU"
9KBMTU	                = "9 KB MTU"
WolCap	                = "Možnosti zapnutí počítače přes síť"
None	                = "Žádný"
PatternMatch	        = "Shoda řetězce"
MagicPacket	        = "Magic Packet"
PatternAndMagic        	= "Shoda řetězce a Magic Packet"
AutoLinkDownPcieMacOff	= "Automatická deaktivace PCIe (Úsporný režim)"
AutoLinkDownPhyOff	= "Automatická deaktivace PHY (Úsporný režim)"
Battery	                = "Povoleno, baterie"
AcBattery	        = "Povoleno, baterie nebo AC"
GreenEthernet           = "Zelený Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Croatian
[Strings.041a]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/p VLAN dodavanje oznaka"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Kontrolni zbroj na periferiju"
LargesendOffload	= "Slanje velikog na periferiju "
SpeedDuplexMode		= "Brzina i dupleks"
auto_nego		= "Automatsko prilagođivanje"
sd10half		= "10 Mb/s poludupleks"
sd10full		= "10 Mb/s puni dupleks"
sd100half		= "100 Mb/s poludupleks"
sd100full		= "100 Mb/s puni dupleks"
sd1000full		= "1.0 Gb/s puni dupleks"
NetworkAddress		= "Mrežna adresa"
JumboFrame		= "Jumbo okvir"
;TxDescNumber		= "Broj Tx opisnika"
RxDescNumber		= "Broj Rx opisnika"
;TxHPQDescNumber	= "Broj Tx opisnika visokog prioriteta"
FlowControl		= "Kontrola protoka"
;AutoSpeedDown		= "Automatsko smanjivanje brzine"
S5WakeOnLan		= "Isključivanje funkcije Probudi se na mreži nakon isključivanja"
10MbFirst               = "Prvo 10 Mb/s"
100MbFirst              = "Prvo 100 Mb/s"
NotSpeedDown            = "Nema smanjivanja brzine"
WolShutdownLinkSpeed    = "Brzina veze za WOL i isključivanje"
AutoCrossoverDet        = "Automatska detekcija preslušavanja"
Disabled                = "Onemogućeno"
Enabled                 = "Omogućeno"
TxEnabled               = "Tx omogućeno"
RxEnabled               = "Rx omogućeno"
RxTxEnabled             = "Rx & Tx omogućeno"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Mogućnosti Probudi se na mreži"
None                    = "Nema"
PatternMatch            = "Podudarnost obrasca"
MagicPacket             = "Magični paket"
PatternAndMagic         = "Podudarnost obrasca i magični paket"
AutoLinkDownPcieMacOff  = "Automatsko isključivanje PCIe (Štednja energije)"
AutoLinkDownPhyOff      = "Automatsko isključivanje PHY (Štednja energije)"
Battery                 = "Omogućeno, baterija"
AcBattery               = "Omogućeno, baterije ili AC"
GreenEthernet           = "Zeleni Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Danish
[Strings.0406]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "Lokalt netværk 802.1Q/1p-mærkning"
;VLanID			= "Lokalt netværk 802.1Q-id"
ChecksumOffload		= "Aflastning af kontrolsum"
LargesendOffload	= "Aflastning af stor forsendelse"
SpeedDuplexMode		= "Hastighed og duplex"
auto_nego		= "Automatisk forhandling"
sd10half		= "10 Mbps halv duplex"
sd10full		= "10 Mbps fuld duplex"
sd100half		= "100 Mbps halv duplex"
sd100full		= "100 Mbps fuld duplex"
sd1000full		= "1.0 Gbps fuld duplex"
NetworkAddress		= "Netværksadresse"
JumboFrame		= "Jumboramme"
;TxDescNumber		= "Antal afsendelsesbuffere"
RxDescNumber		= "Antal modtagelsesbeskrivelser"
;TxHPQDescNumber	= "Antal høj prioritet afsendelsesbuffere"
FlowControl		= "Flow-kontrol"
;AutoSpeedDown		= "Auto-hastighed ned"
S5WakeOnLan		= "Nedluk Wake-On-Lan"
10MbFirst               = "10 Mbps først"
100MbFirst              = "100 Mbps først"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "Hastighed for Wake-On-Lan og nedlukningsforbindelse"
AutoCrossoverDet        = "Detektering af automatisk crossover"
Disabled                = "Deaktiver"
Enabled                 = "Aktiver"
TxEnabled               = "Tx aktiveret"
RxEnabled               = "Rx aktiveret"
RxTxEnabled             = "Rx og Tx aktiveret"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "Automatisk deaktivering af PCIe (StrømStyring)"
AutoLinkDownPhyOff      = "Automatisk deaktivering af PHY (StrømStyring)"
Battery                 = "Aktiveret, batteri"
AcBattery               = "Aktiveret, batteri eller AC"
GreenEthernet           = "Grøn Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Dutch_Standard
[Strings.0413]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p VLAN-tagging"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Controlesom-offload"
LargesendOffload	= "Grote verzendings-offload"
SpeedDuplexMode		= "Snelheid & Duplex"
auto_nego		= "Automatische onderhandeling"
sd10half		= "10 Mbps, half-duplex"
sd10full		= "10 Mbps, full-duplex"
sd100half		= "100 Mbps, half-duplex"
sd100full		= "100 Mbps, full-duplex"
sd1000full		= "1,0 Gbps, full-duplex"
NetworkAddress		= "Netwerkadres"
JumboFrame		= "Jumboframe"
;TxDescNumber		= "Nummer van Tx-descriptor"
RxDescNumber		= "Nummer van Rx-descriptor"
;TxHPQDescNumber	= "Nummer van Tx-descriptor hoge prioriteit"
FlowControl		= "Datatransportbesturing"
;AutoSpeedDown		= "Automatisch snelheid omlaag"
S5WakeOnLan		= "Wake-on-lan afsluiten"
10MbFirst               = "10 Mbps eerst"
100MbFirst              = "100 Mbps eerst"
NotSpeedDown            = "Niet snelheid omlaag"
WolShutdownLinkSpeed    = "Snelheid verbinding afsluiten & WOL"
AutoCrossoverDet        = "Automatische detectie cross-over"
Disabled                = "Uitgeschakeld"
Enabled                 = "Ingeschakeld"
TxEnabled               = "Tx ingeschakeld"
RxEnabled               = "Rx ingeschakeld"
RxTxEnabled             = "Rx & Tx ingeschakeld"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Mogelijkheden wake-on-lan"
None                    = "Geen"
PatternMatch            = "Patroonovereenkomst"
MagicPacket             = "Magisch pakket"
PatternAndMagic         = "Patroonovereenkomst & Magisch pakket"
AutoLinkDownPcieMacOff  = "PCIe automatisch uitschakelen (energiebesparing)"
AutoLinkDownPhyOff      = "PHY automatisch uitschakelen (energiebesparing)"
Battery                 = "Ingeschakeld, batterij"
AcBattery               = "Ingeschakeld, batterij of AC"
GreenEthernet           = "Groen Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Finnish
[Strings.040b]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Virtuaalisen lähiverkon merkitseminen"
;VLanID			= "802.1Q Virtuaalisen lähiverkon tunniste"
ChecksumOffload		= "Pura tarkistussumma"
LargesendOffload	= "Pura isot lähetykset"
SpeedDuplexMode		= "Nopeus & Duplex"
auto_nego		= "Automaattinen neuvottelu"
sd10half		= "10 Mbps puolikas Duplex"
sd10full		= "10 Mbps täysi Duplex"
sd100half		= "100 Mbps puolikas Duplex"
sd100full		= "100 Mbps täysi Duplex"
sd1000full		= "1.0 Gbps täysi Duplex"
NetworkAddress		= "Verkon osoite"
JumboFrame		= "Jumbo Frame"
;TxDescNumber		= "Siirrettävien deskriptoreiden määrä"
RxDescNumber		= "Vastaanotettavien deskriptoreiden määrä"
;TxHPQDescNumber	= "Etusijalla olevien siirrettävien deskriptoreiden määrä"
FlowControl		= "Datavuon ohjaus"
;AutoSpeedDown		= "Automaattinen nopeuden vähennys"
S5WakeOnLan		= "Sammuta herätystoiminto Lanin kautta"
10MbFirst               = "10 Mbps ensin"
100MbFirst              = "100 Mbps ensin"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "Herätystoiminto Lanin kautta & linkkinopeuden sammutus"
AutoCrossoverDet        = "Automaattinen ohitustunnistin"
Disabled                = "Poista käytöstä"
Enabled                 = "Ota käyttöön"
TxEnabled               = "Tx Käytössä"
RxEnabled               = "Rx Käytössä"
RxTxEnabled             = "Rx & Tx Käytössä"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "Ota PCIe automaattisesti pois päältä (Virransäästö)"
AutoLinkDownPhyOff      = "Ota PHY automaattisesti pois päältä (Virransäästö)"
Battery                 = "Käytössä, akku"
AcBattery               = "Käytössä, akku tai verkkovirta"
GreenEthernet           = "Vihreä Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;French_Standard
[Strings.040c]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Etiquette réseau local virtuel"
;VLanID			= "802.1Q Identifiant réseau local virtuel"
ChecksumOffload		= "Somme de contrôle hors charge"
LargesendOffload	= "Grand envoi hors charge"
SpeedDuplexMode		= "Vitesse & Duplex"
auto_nego		= "Négociation auto"
sd10half		= "10 Mbps Semi-duplex"
sd10full		= "10 Mbps Duplex intégral"
sd100half		= "100 Mbps Semi-duplex"
sd100full		= "100 Mbps Duplex intégral"
sd1000full		= "1.0 Gbps Duplex intégral"
NetworkAddress		= "Adresse de réseau"
JumboFrame		= "Cadre jumbo"
;TxDescNumber		= "Nombre de descripteur de transmission"
RxDescNumber		= "Nombre de descripteur de réception "
;TxHPQDescNumber	= "Nombre de descripteur de transmission haute priorité "
FlowControl		= "Contrôle de flux"
;AutoSpeedDown		= "Ralentir auto vitesse"
S5WakeOnLan		= "Arrêter Réveil par réseau"
10MbFirst               = "10 Mbps en premier"
100MbFirst              = "100 Mbps en premier"
NotSpeedDown            = "Fonctions Réveil par le réseau"
WolShutdownLinkSpeed    = "Vitesse de lien Réveil par réseau & Arrêt"
AutoCrossoverDet        = "Détection auto inversion"
Disabled                = "Désactiver"
Enabled                 = "Activer"
TxEnabled               = "Tx activé"
RxEnabled               = "Rx activé"
RxTxEnabled             = "Rx & Tx activé"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Fonctions Réveil par le réseau"
None                    = "Aucun"
PatternMatch            = "Correspondance au modèle"
MagicPacket             = "Paquet Magic"
PatternAndMagic         = "Correspondance au modèle et Paquet Magic"
AutoLinkDownPcieMacOff  = "Désactiver auto PCIe (Economie énergie)"
AutoLinkDownPhyOff      = "Désactiver auto PHY (Economie énergie)"
Battery                 = "Activé, Batterie"
AcBattery               = "Activé, Batterie ou AC"
GreenEthernet           = "Ethernet vert"


;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;German_Standard
[Strings.0407]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Klassifizierung des virtuellen, lokalen Netzwerks"
;VLanID			= "802.1Q Identifikator des virtuellen, lokalen Netzwerks"
ChecksumOffload		= "Prüfsummenabladung"
LargesendOffload	= "Abladung großer Übertragung"
SpeedDuplexMode		= "Geschwindigkeit & Duplex"
auto_nego		= "Autom. Aushandlung"
sd10half		= "10 Mbit/s Halbduplex"
sd10full		= "10 Mbit/s Vollduplex"
sd100half		= "100 Mbit/s Halbduplex"
sd100full		= "100 Mbit/s Vollduplex"
sd1000full		= "1.0 Gbit/s Vollduplex"
NetworkAddress		= "Netzwerkadresse"
JumboFrame		= "Jumbo-Rahmen"
;TxDescNumber		= "Nummer des Übertragungs-Deskriptors"
RxDescNumber		= "Nummer des Empfangs-Deskriptors"
;TxHPQDescNumber	= "Nummer des Übertragungs-Deskriptors mit hoher Priorität"
FlowControl		= "Fließkontrolle"
;AutoSpeedDown		= "Autom. verlangsamen"
S5WakeOnLan		= "Wake-On-Lan herunterfahren"
10MbFirst               = "10 Mbit/s zuerst"
100MbFirst              = "100 Mbit/s zuerst"
NotSpeedDown            = "Nicht verlangsamen"
WolShutdownLinkSpeed    = "Wake-On-Lan & Link-Geschwindigkeit herunterfahren"
AutoCrossoverDet        = "Autom. Crossover-Erkennung"
Disabled                = "Deaktivieren"
Enabled                 = "Aktivieren"
TxEnabled               = "Tx aktiviert"
RxEnabled               = "Rx deaktiviert"
RxTxEnabled             = "Rx & Tx aktiviert"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-LAN-Funktionen"
None                    = "Kein"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "PCIe autom. deaktivieren (Energie sparen)"
AutoLinkDownPhyOff      = "PHY autom. deaktivieren (Energie sparen)"
Battery                 = "Aktiviert, Batterie"
AcBattery               = "Aktiviert, Batterie oder Netz"
GreenEthernet           = "Green-Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"
;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Greek
[Strings.0408]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "Κωδικοποίηση εικονικού τοπικού δικτύου 802.1Q/1p"
;VLanID			= "Αναγνωριστικό εικονικού τοπικού δικτύου 802.1Q/1p"
ChecksumOffload		= "Μείωση φόρτου αθροίσματος ελέγχου"
LargesendOffload	= "Μείωση φόρτου μεγάλης αποστολής"
SpeedDuplexMode		= "Ταχύτητα & Αμφίδρομη"
auto_nego		= "Αυτόματη διαπραγμάτευση"
sd10half		= "10Mbps/Ημι-αμφίδρομη"
sd10full		= "10Mbps/Πλήρως αμφίδρομη"
sd100half		= "100Mbps/Ημι-αμφίδρομη"
sd100full		= "100Mbps/Πλήρως αμφίδρομη"
sd1000full		= "1.0 Gbps/Πλήρως αμφίδρομη"
NetworkAddress		= "Διεύθυνση δικτύου"
JumboFrame		= "Πλαίσιο Jumbo"
;TxDescNumber		= "Αριθμός περιγραφών μετάδοσης"
RxDescNumber		= "Αριθμός περιγραφών παραλαβής"
;TxHPQDescNumber	= "Αριθμός περιγραφών μετάδοσης υψηλής προτεραιότητας"
FlowControl		= "Έλεγχος ροής"
;AutoSpeedDown		= "Αυτόματη μείωση ταχύτητας"
S5WakeOnLan		= "Wake-on-LAN τερματισμού"
10MbFirst               = "Πρώτα 10 Mbps "
100MbFirst              = "Πρώτα 100 Mbps"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "Wake-on-LAN & ταχύτητα σύνδεσης τερματισμού"
AutoCrossoverDet        = "Αυτόματη ανίχνευση τιμής διασταύρωσης"
Disabled                = "Απενεργοποίηση"
Enabled                 = "Ενεργοποίηση"
TxEnabled               = "Ενεργοποιημένο Tx"
RxEnabled               = "Ενεργοποιημένο Rx"
RxTxEnabled             = "Ενεργοποιημένο Rx & Tx"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "PCIe αυτόματης απενεργοποίησης (Εξοικονόμηση ενέργειας)"
AutoLinkDownPhyOff      = "PHY αυτόματης απενεργοποίησης (Εξοικονόμηση ενέργειας)"
Battery                 = "Ενεργοποίηση, Μπαταρία"
AcBattery               = "Ενεργοποίηση, Μπαταρία ή AC"
GreenEthernet           = "Green Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Hebrew
[Strings.040d]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "תיוג וירטואלי לרשת 802.1Q/1p LAN"
;VLanID			= "מזהה וירטואלי לרשת 802.1Q LAN"
ChecksumOffload		= "העברת סיכום ביקורת"
LargesendOffload	= "העברת שליחה גדולה"
SpeedDuplexMode		= "מהירות וכיווניות"
auto_nego		= "משא ומתן אוטומטי"
sd10half		= "10Mbps חד כיווני"
sd10full		= "10Mbps דו כיווני"
sd100half		= "100Mbps חד כיווני"
sd100full		= "100Mbps דו כיווני"
sd1000full		= "1.0 Gbps דו כיווני"
NetworkAddress		= "כתובת רשת"
JumboFrame		= "מסגרת Jumbo"
;TxDescNumber		= "מספר מתאר שידור"
RxDescNumber		= "מספר מתאר קליטה"
;TxHPQDescNumber	= "מספר מתאר שידור בעדיפות גבוהה"
FlowControl		= "בקרת זרימה"
;AutoSpeedDown		= "האטה אוטומטית"
S5WakeOnLan		= "כיבוי Wake-On-Lan"
10MbFirst               = "10Mbps ראשון"
100MbFirst              = "100Mbps ראשון"
NotSpeedDown            = "ללא האטה"
WolShutdownLinkSpeed    = "מהירות קישור Wake-On-Lan וכיבוי"
AutoCrossoverDet        = "גילוי אוטומטי של חיבור מוצלב"
Disabled                = "בטל"
Enabled                 = "אפשר"
TxEnabled               = "שידור מאופשר"
RxEnabled               = "קליטה מאופשרת"
RxTxEnabled             = "שידור וקליטה מאופשרים"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "יכולות Wake-On-Lan"
None                    = "ללא"
PatternMatch            = "התאמת תבנית"
MagicPacket             = "מנת קסם"
PatternAndMagic         = "התאמת תבנית ומנת קסם"
AutoLinkDownPcieMacOff  = "ביטול אוטומטי של PowerSaving) PCIe)"
AutoLinkDownPhyOff      = "ביטול אוטומטי של PowerSaving) PHY)"
Battery                 = "מאופשר, סוללה"
AcBattery               = "מאופשר, סוללה או מתח חילופין (AC)"
GreenEthernet           = "ירוקEthernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Hungarian
[Strings.040e]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Virtuális helyi hálózati (VLAN) címkézés"
;VLanID			= "802.1Q Virtuális helyi hálózati (VLAN) azonosító"
ChecksumOffload		= "Ellenőrzőösszeg tehermentesítése"
LargesendOffload	= "Nagyobb küldemény tehermentesítése"
SpeedDuplexMode		= "Sebesség és duplex"
auto_nego		= "Automatikus sebesség- és duplexitás-felismerés"
sd10half		= "10 Mbps Félduplex"
sd10full		= "10 Mbps Teljes duplex"
sd100half		= "100 Mbps Mbps Félduplex"
sd100full		= "100 Mbps Teljes duplex"
sd1000full		= "1.0 Gbps Teljes duplex"
NetworkAddress		= "Hálózati cím"
JumboFrame		= "Jumbo Frame (Óriás keret)"
;TxDescNumber		= "Átviteli leíró száma"
RxDescNumber		= "Vételi leíró száma"
;TxHPQDescNumber	= "Magas prioritású átviteli leíró száma"
FlowControl		= "Áramlásszabályozás"
;AutoSpeedDown		= "Automatikus sebességcsökkentés"
S5WakeOnLan		= "Felélesztés leállítás után hálózaton keresztül"
10MbFirst               = "10 Mbps First"
100MbFirst              = "100 Mbps First"
NotSpeedDown            = "Nincs lassítás"
WolShutdownLinkSpeed    = "Felélesztés a hálózaton keresztül és leállítás kapcsolati sebessége"
AutoCrossoverDet        = "Keresztezés automatikus észlelése"
Disabled                = "Letiltás"
Enabled                 = "Engedélyezés"
TxEnabled               = "Tx Engedélyezve"
RxEnabled               = "Rx Engedélyezve"
RxTxEnabled             = "Rx és Tx Engedélyezve"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Hálózaton keresztül történő felélesztéssel kapcsolatos funkciók"
None                    = "Nincs"
PatternMatch            = "Mintaillesztés"
MagicPacket             = "Megfelelő csomag"
PatternAndMagic         = "Mintaillesztés és megfelelő csomag"
AutoLinkDownPcieMacOff  = "PCIe automatikus letiltása (Energiatakarékos)"
AutoLinkDownPhyOff      = "PHY automatikus letiltása (Energiatakarékos)"
Battery                 = "Engedélyezve, akkumulátor"
AcBattery               = "Engedélyezve, akkumulátor vagy AC"
GreenEthernet           = "Energiatakarékos Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Italian_Standard
[Strings.0410]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Tagging di Virtual Local Area Network"
;VLanID			= "802.1Q Identificatore di Virtual Local Area Network"
ChecksumOffload		= "Checksum Offload"
LargesendOffload	= "Large Send Offload"
SpeedDuplexMode		= "Velocità e duplex"
auto_nego		= "Auto Negotiation"
sd10half		= "10 Mbps Half Duplex"
sd10full		= "10 Mbps Full Duplex"
sd100half		= "100 Mbps Half Duplex"
sd100full		= "100 Mbps Full Duplex"
sd1000full		= "1.0 Gbps Full Duplex"
NetworkAddress		= "Indirizzo di rete"
JumboFrame		= "Jumbo Frame"
;TxDescNumber		= "Numero di descrittore trasmissione"
RxDescNumber		= "Numero di descrittore ricezione"
;TxHPQDescNumber	= "Numero di descrittore trasmissione alta priorità"
FlowControl		= "Controllo flusso"
;AutoSpeedDown		= "Rallentamento automatico"
S5WakeOnLan		= "Shutdown Wake-On-Lan"
10MbFirst               = "Prima 10 Mbps"
100MbFirst              = "Prima 100 Mbps"
NotSpeedDown            = "Non rallentamento"
WolShutdownLinkSpeed    = "WOL & Shutdown Link Speed"
AutoCrossoverDet        = "Rilevamento automatico crossover"
Disabled                = "Disabilita"
Enabled                 = "Abilita"
TxEnabled               = "Tx Abilitata"
RxEnabled               = "Rx Abilitata"
RxTxEnabled             = "Rx & Tx Abilitata"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Funzioni Wake-On-Lan"
None                    = "Nessuno"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match e Magic Packet"
AutoLinkDownPcieMacOff  = "Disabilitazione automatica PCIe (risparmio energia)"
AutoLinkDownPhyOff      = "Disabilitazione automatica PHY (risparmio energia)"
Battery                 = "Abilitato, batteria"
AcBattery               = "Abilitato, batteria o AC"
GreenEthernet           = "Green Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Japanese
[Strings.0411]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p ヴァーチャルLANタギング"
;VLanID			= "802.1Q ヴァーチャルLAN識別子"
ChecksumOffload		= "チェックサムオフロード"
LargesendOffload	= "一括送信オフロード"
SpeedDuplexMode		= "速度とデュプレックス"
auto_nego		= "自動ネゴシエーション"
sd10half		= "10 Mbps ハーフデュプレックス"
sd10full		= "10 Mbps フルデュプレックス"
sd100half		= "100 Mbps ハーフデュプレックス"
sd100full		= "100 Mbps フルデュプレックス"
sd1000full		= "1.0 Gbps フルデュプレックス"
NetworkAddress		= "ネットワークアドレス"
JumboFrame		= "ジャンボフレーム"
;TxDescNumber		= "伝送識別子の数"
RxDescNumber		= "受信識別子の数"
;TxHPQDescNumber	= "高優先度伝送識別子の数"
FlowControl		= "フローコントロール"
;AutoSpeedDown		= "自動速度ダウン"
S5WakeOnLan		= "LAN 上のウェークアップのシャットダウン"
10MbFirst               = "10 Mbps 優先"
100MbFirst              = "100 Mbps 優先"
NotSpeedDown            = "速度低下ではない"
WolShutdownLinkSpeed    = "LAN上Wakeup及びShutdownリンク速度"
AutoCrossoverDet        = "自動クロスオーバー検出"
Disabled                = "無効"
Enabled                 = "有効"
TxEnabled               = "Tx 有効"
RxEnabled               = "Rx 有効"
RxTxEnabled             = "受信と伝送有効"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan機能"
None                    = "なし"
PatternMatch            = "パターン適合"
MagicPacket             = "マジックパケット"
PatternAndMagic         = "パターン適合とマジックパケット"
AutoLinkDownPcieMacOff  = "自動無効 PCIe (節電)"
AutoLinkDownPhyOff      = "自動無効PHY (節電)"
Battery                 = "有効、バッテリ"
AcBattery               = "有効、バッテリまたはAC"
GreenEthernet           = "グリーンイーサネット"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Korean
[Strings.0412]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p VLAN 태깅"
;VLanID			= "802.1Q VLAN 식별자"
ChecksumOffload		= "체크섬 오프로드"
LargesendOffload	= "Large Send Offload"
SpeedDuplexMode		= "속도 및 이중"
auto_nego		= "자동 교섭"
sd10half		= "10 Mbps 반이중"
sd10full		= "10 Mbps 전이중"
sd100half		= "100 Mbps 반이중"
sd100full		= "100 Mbps 전이중"
sd1000full		= "1.0 Gbps 전이중"
NetworkAddress		= "네트워크 주소"
JumboFrame		= "점보 프레임"
;TxDescNumber		= "송신 설명자 수"
RxDescNumber		= "수신 설명자 수"
;TxHPQDescNumber	= "높은 우선 순위 송신 설명자 수"
FlowControl		= "흐름 제어"
;AutoSpeedDown		= "자동 감속"
S5WakeOnLan		= "웨이크 온 랜 종료"
10MbFirst               = "10 Mbps 먼저"
100MbFirst              = "100 Mbps 먼저"
NotSpeedDown            = "속도 저하 안 함"
WolShutdownLinkSpeed    = "웨이크 온 랜 및 종료 링크 속도"
AutoCrossoverDet        = "자동 크로스오버 탐지"
Disabled                = "사용 안 함"
Enabled                 = "사용"
TxEnabled               = "Tx 사용"
RxEnabled               = "Rx 사용"
RxTxEnabled             = "Rx/Tx 사용"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "WOL 기능"
None                    = "없음"
PatternMatch            = "패턴 매치"
MagicPacket             = "매직 패킷"
PatternAndMagic         = "패턴 매치와 매직 패킷"
AutoLinkDownPcieMacOff  = "PCIe 자동 비활성화(절전)"
AutoLinkDownPhyOff      = "PHY 자동 비활성화(절전)"
Battery                 = "사용, 전지"
AcBattery               = "사용, 전지 또는 AC"
GreenEthernet           = "절전형 이더넷"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Norwegian_Bokmal
[Strings.0414]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Tagging av virtuelt lokalnettverk"
;VLanID			= "802.1Q Identifikator for virtuelt lokalnettverk"
ChecksumOffload		= "Sjekksum avlastning"
LargesendOffload	= "sending avlastning"
SpeedDuplexMode		= "Hastighet og dupleks"
auto_nego		= "Automatisk forhandling"
sd10half		= "10Mbps Halv dupleks"
sd10full		= "10Mbps Full dupleks"
sd100half		= "100Mbps Halv dupleks"
sd100full		= "100Mbps Full dupleks"
sd1000full		= "1.0 Gbps Full dupleks"
NetworkAddress		= "Nettverksadresse"
JumboFrame		= "Jumbo-ramme"
;TxDescNumber		= "Antall overføringsbetegnelser"
RxDescNumber		= "Antall mottaksbetegnelser"
;TxHPQDescNumber	= "Antall overføringsbetegnelser med høy prioritet"
FlowControl		= "Flytkontroll"
;AutoSpeedDown		= "Automatisk hastighet ned"
S5WakeOnLan		= "Avslutningsaktivering på nettverk"
10MbFirst               = "10 Mbps Først"
100MbFirst              = "100 Mbps Først"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "Reaktivering på nettverk og avslutningslinjehastighet"
AutoCrossoverDet        = "Automatisk registrering av grenbytte"
Disabled                = "Deaktiver"
Enabled                 = "Aktiver"
TxEnabled               = "Tx aktivert"
RxEnabled               = "Rx aktivert"
RxTxEnabled             = "Rx og Tx aktivert"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "Automatisk deaktivere PCIe (strømsparing)"
AutoLinkDownPhyOff      = "Automatisk deaktivere PHY (strømsparing)"
Battery                 = "Aktivert, batteri"
AcBattery               = "Aktivert, batteri or vekselstrøm"
GreenEthernet           = "Grønt Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Polish
[Strings.0415]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Oznaczenie wirtualnej lokalnej sieci komputerowej"
;VLanID			= "802.1Q Identyfikator wirtualnej lokalnej sieci komputerowej"
ChecksumOffload		= "Suma kontrolna bez obciążenia"
LargesendOffload	= "Large Send Offload"
SpeedDuplexMode		= "Szybkość i dupleks"
auto_nego		= "Automatyczna negocjacja"
sd10half		= "10 Mbps Half Duplex"
sd10full		= "10 Mbps Full Duplex"
sd100half		= "100 Mbps Half Duplex"
sd100full		= "100 Mbps Full Duplex"
sd1000full		= "1.0 Gbps Full Duplex"
NetworkAddress		= "Adres sieciowy"
JumboFrame		= "Ramka Jumbo"
;TxDescNumber		= "Liczba deskryptora transmisji"
RxDescNumber		= "Liczba deskryptora odbioru"
;TxHPQDescNumber	= "Liczba deskryptora wysokiego priorytetu transmisji"
FlowControl		= "Sterowanie przepływem"
;AutoSpeedDown		= "Automatyczne zmniejszenie szybkości"
S5WakeOnLan		= "Zamknięcie Wybudzanie przy uaktywnieniu sieci"
10MbFirst               = "Pierwsze 10 Mbps"
100MbFirst              = "Pierwsze 100 Mbps"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "Wybudzanie przy uaktywnieniu sieci i Szybkość zamykania łącza"
AutoCrossoverDet        = "Autodetekcja rodzaju połączenia"
Disabled                = "Wyłącz"
Enabled                 = "Włącz"
TxEnabled               = "Włączone Tx"
RxEnabled               = "Włączone Rx"
RxTxEnabled             = "Włączone Rx i Tx"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "Automatyczne wyłączenie PCIe (Oszczędzanie energii)"
AutoLinkDownPhyOff      = "Automatyczne wyłączanie PHY (Oszczędzanie energii)"
Battery                 = "Włączone, bateria"
AcBattery               = "Włączone, bateria lub prąd zmienny"
GreenEthernet           = "Energooszczędny Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Portuguese_Brazilian
[Strings.0416]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Etiquetagem de Rede de Área Local Virtual"
;VLanID			= "802.1Q Identificador de Rede de Área Local Virtual"
ChecksumOffload		= "Descarga de Checksum"
LargesendOffload	= "Descarga Large Send"
SpeedDuplexMode		= "Velocidade & Duplex"
auto_nego		= "Auto Negociação"
sd10half		= "10 Mbps Half Duplex"
sd10full		= "10 Mbps Full Duplex"
sd100half		= "100 Mbps Half Duplex"
sd100full		= "100 Mbps Full Duplex"
sd1000full		= "1.0 Gbps Full Duplex"
NetworkAddress		= "Endereço de Rede"
JumboFrame		= "Jumbo Frame"
;TxDescNumber		= "Número do Descritor de Transmissão"
RxDescNumber		= "Número do Descritor de Recepção"
;TxHPQDescNumber	= "Número do Descritor de Transmissão de Alta Prioridade"
FlowControl		= "Controlo de Fluxo"
;AutoSpeedDown		= "Velocidade Automática Desactivada"
S5WakeOnLan		= "Desligar Despertar Aquando de Lan"
10MbFirst               = "10 Mbps Primeiro"
100MbFirst              = "100 Mbps Primeiro"
NotSpeedDown            = "Não reduzir velocidade"
WolShutdownLinkSpeed    = "Despertar Aquando de Lan & Velocidade de Ligação Desligar"
AutoCrossoverDet        = "Detecção Auto Crossover"
Disabled                = "Desactivar"
Enabled                 = "Activar"
TxEnabled               = "Tx Activado"
RxEnabled               = "Rx Activado"
RxTxEnabled             = "Rx & Tx Activados"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Capacidades Wake-On-Lan"
None                    = "Nenhum"
PatternMatch            = "Correspondência de padrões"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Correspondência de pacotes e Magic Packet"
AutoLinkDownPcieMacOff  = "Auto Desactivar PCIe (Poupança de Energia)"
AutoLinkDownPhyOff      = "Auto Desactivar PHY (Poupança de Energia)"
Battery                 = "Activado, Bateria"
AcBattery               = "Activado, Bateria ou CA"
GreenEthernet           = "Ethernet Verde"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

; Portuguese_Standard
[Strings.0816]
Realtek                  = "Realtek"
VLanTagging		= "802.1Q/1p VLAN com etiqueta"
;VLanID			= "ID da VLAN 802.1Q"
ChecksumOffload		= "Soma de verificação offload"
LargesendOffload	= "Envio grande de offload"
SpeedDuplexMode		= "Velocidade e modo duplex"
auto_nego		= "Auto negociação"
sd10half		= "10 Mbps modo semi duplex"
sd10full		= "10 Mbps modo full-duplex"
sd100half		= "100 Mbps modo semi duplex"
sd100full		= "100 Mbps modo full-duplex"
sd1000full		= "1,0 Gbps modo full-duplex"
NetworkAddress		= "Endereço de rede"
JumboFrame		= “Estrutura jumbo”
;TxDescNumber		= "Número do descritor de transmissão"
RxDescNumber		= "Número do descritor de recepção"
;TxHPQDescNumber	= "Número do descritor de transmissão de alta prioridade"
FlowControl		= “Controlo do fluxo”
;AutoSpeedDown		= "Diminuição automática da velocidade"
S5WakeOnLan		= “Encerrar Wake-On-Lan”
10MbFirst                = "10 Mbps primeiro"
100MbFirst                = "100 Mbps primeiro"
NotSpeedDown             = "Não diminuir velocidade"
WolShutdownLinkSpeed     = "WOL e encerrar velocidade de ligação"
AutoCrossoverDet         = "Detecção cruzada automática"
Disabled                 = "Desactivado"
Enabled                  = "Activado"
TxEnabled                = "Transmissão activada"
RxEnabled                = "Recepção activada"
RxTxEnabled              = "Recepção e transmissão activada"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
WolCap                   = "Capacidades Wake-On-Lan"
None                     = "Nenhuma"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match e Magic Packet"
AutoLinkDownPcieMacOff       = "Desactivar PCIe automaticamente (poupança de energia)"
AutoLinkDownPhyOff       = "Desactivar PHY automaticamente (poupança de energia)"
Battery                  = "Activada, bateria"
AcBattery                = "Activada, bateria ou a.c."
GreenEthernet            = "Ethernet verde"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Romanian
[Strings.0418]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "Etichetare VLAN 802.1Q/1p"
;VLanID			= "Identitate VLAN 802.1Q"
ChecksumOffload		= "Preluare sarcină de verificare erori"
LargesendOffload	= "Preluare sarcină de trimitere pachete mari"
SpeedDuplexMode		= "Viteză şi duplex"
auto_nego		= "Negociere automată"
sd10half		= "10 Mbps semiduplex"
sd10full		= "10 Mbps duplex"
sd100half		= "100 Mbps semiduplex"
sd100full		= "100 Mbps duplex"
sd1000full		= "1,0 Gbps duplex"
NetworkAddress		= "Adresă de reţea"
JumboFrame		= "Cadru jumbo"
;TxDescNumber		= "Număr descriptor Tx"
RxDescNumber		= "Număr descriptor Rx"
;TxHPQDescNumber	= "Număr descriptor Tx prioritate mare"
FlowControl		= "Control debit"
;AutoSpeedDown		= "Reducere automată viteză"
S5WakeOnLan		= "Dezactivare trezire prin LAN"
10MbFirst               = "10 Mbps iniţial"
100MbFirst              = "100 Mbps iniţial"
NotSpeedDown            = "Fără reducere viteză"
WolShutdownLinkSpeed    = "WOL şi dezactivare viteză legătură"
AutoCrossoverDet        = "Detectare automată simulare modem"
Disabled                = "Dezactivat"
Enabled                 = "Activat"
TxEnabled               = "Tx activat"
RxEnabled               = "Rx activat"
RxTxEnabled             = "Rx şi Tx activat"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Capacităţi de trezire prin LAN"
None                    = "Niciunul"
PatternMatch            = "Potrivire model"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Potrivire model şi Magic Packet"
AutoLinkDownPcieMacOff  = "Dezactivare automată PCIe (Economie de energie)"
AutoLinkDownPhyOff      = "Dezactivare automată PHY (Economie de energie)"
Battery                 = "Activat, baterie"
AcBattery               = "Activat, baterie sau AC"
GreenEthernet           = "Ethernet verde"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Russian
[Strings.0419]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "Тегирование 802.1Q/1p VLAN"
;VLanID			= "Идентификатор 802.1Q VLAN"
ChecksumOffload		= "Контрольная сумма разгрузки"
LargesendOffload	= "Разгрузка при большой отправке"
SpeedDuplexMode		= "Скорость и дуплекс"
auto_nego		= "Автосогласование"
sd10half		= "10 Мбит/с полудуплекс"
sd10full		= "10 Мбит/с дуплекс"
sd100half		= "100 Мбит/с полудуплекс"
sd100full		= "100 Мбит/с дуплекс"
sd1000full		= "1 Гбит/с дуплекс"
NetworkAddress		= "Сетевой адрес"
JumboFrame		= "Большой кадр"
;TxDescNumber		= "Число дескриптора Tx"
RxDescNumber		= "Число дескриптора Rx"
;TxHPQDescNumber	= "Число дескриптора Tx с высоким приоритетом"
FlowControl		= "Управление потоком"
;AutoSpeedDown		= "Автопонижение скорости"
S5WakeOnLan		= "Включение по локальной сети после отключения"
10MbFirst               = "Сначала 10 Mбит/с"
100MbFirst              = "Сначала 100 Mбит/с"
NotSpeedDown            = "Не использовать автопонижение скорости"
WolShutdownLinkSpeed    = "Скорость при включении по локальной сети после отключения"
AutoCrossoverDet        = "Автоопределение кросс-кабеля"
Disabled                = "Выкл"
Enabled                 = "Вкл"
TxEnabled               = "Контрольная сумма Tx"
RxEnabled               = "Контрольная сумма Rx"
RxTxEnabled             = "Контрольная сумма Tx/Rx"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Функции включения по сети"
None                    = "Нет"
PatternMatch            = "Соответствие шаблону"
MagicPacket             = "Специальный пакет"
PatternAndMagic         = "Соответствие шаблону И Специальный пакет"
AutoLinkDownPcieMacOff  = "Автоотключение PCIe (энергосбережение)"
AutoLinkDownPhyOff      = "Автоотключение PHY (энергосбережение)"
Battery                 = "Вкл, батарея"
AcBattery               = "Вкл, батарея или пер. ток"
GreenEthernet           = "Зеленый Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Slovenian
[Strings.0424]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Označevanje virtualnega lokalnega omrežja"
;VLanID			= "802.1Q Identifikator virtualnega lokalnega omrežja"
ChecksumOffload		= "Razbremenitev kontrolne vsote"
LargesendOffload	= "Razbremenitev velikega prenosa"
SpeedDuplexMode		= "Hitrost in dupleks"
auto_nego		= "Samopogajanje"
sd10half		= "10 Mb/s Polovični dupleks"
sd10full		= "10 Mb/s Polni dupleks"
sd100half		= "100 Mb/s Polovični dupleks"
sd100full		= "100 Mb/s Polni dupleks"
sd1000full		= "1.0 Gb/s Polni dupleks"
NetworkAddress		= "Omrežni naslov"
JumboFrame		= "Jumbo okvir"
;TxDescNumber		= "Številka prenosa deskriptorja"
RxDescNumber		= "Številka oddajneqa deskriptorja"
;TxHPQDescNumber	= "Številka visoko prioritetnega prenosnega deskriptorja"
FlowControl		= "Kontrola pretoka"
;AutoSpeedDown		= "Samodejna upočasnitev"
S5WakeOnLan		= "Zaustavitev Bujenje-na-Lan"
10MbFirst               = "10 Mb/s Najprej"
100MbFirst              = "100 Mb/s Najprej"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "Bujenje-na-Lan in zaustavitev hitrosti povezave"
AutoCrossoverDet        = "Samodejno križno zaznavanje"
Disabled                = ''Onemogoči''
Enabled                 = "Omogoči"
TxEnabled               = "Tx Omogočeno"
RxEnabled               = "Rx Omogočeno"
RxTxEnabled             = "Rx in Tx omogočeno"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "Samodejno onemogočenje PCIe (Varčevanje z energijo)"
AutoLinkDownPhyOff      = "Samodejno onemogočenje PHY (Varčevanje z energijo)"
Battery                 = "Omogočeno, baterija"
AcBattery               = "Omogočeno, baterija ali AC"
GreenEthernet           = "Zeleni Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Spanish_Traditional_Sort
[Strings.040a]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "Etiquetado de red de área local virtual 802.1Q/1p"
;VLanID			= "Identificador de red de área local virtual 802.1Q"
ChecksumOffload		= "Descarga de suma de comprobación"
LargesendOffload	= "Descarga de gran envío"
SpeedDuplexMode		= "Velocidad y Dúplex"
auto_nego		= "Negociación automática"
sd10half		= "10 Mbps Half Dúplex"
sd10full		= "10 Mbps Full Dúplex"
sd100half		= "100 Mbps Half Dúplex"
sd100full		= "100 Mbps Full Dúplex"
sd1000full		= "1.0 Gbps Full Dúplex"
NetworkAddress		= "Dirección de red"
JumboFrame		= "Trama Jumbo"
;TxDescNumber		= "Número del descriptor de transmisión"
RxDescNumber		= "Número del descriptor de recepción"
;TxHPQDescNumber	= "Número de descriptor de transmisión de alta prioridad"
FlowControl		= "Control de flujo"
;AutoSpeedDown		= "Descenso automático de velocidad"
S5WakeOnLan		= "Activación con LAN de apagado"
10MbFirst               = "10 Mbps primero"
100MbFirst              = "100 Mbps primero"
NotSpeedDown            = "Sin reducción de velocidad"
WolShutdownLinkSpeed    = "Velocidad de enlace de activación con LAN y apagado"
AutoCrossoverDet        = "Detección automática de cruce"
Disabled                = "Desactivar"
Enabled                 = "Activar"
TxEnabled               = "Tx activada"
RxEnabled               = "Rx activada"
RxTxEnabled             = "Rx y Tx activado"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Funciones Wake-On-Lan"
None                    = "Ninguno"
PatternMatch            = "Comparar patrón"
MagicPacket             = "Paquete mágico"
PatternAndMagic         = "Comparar patrón y paquete mágico"
AutoLinkDownPcieMacOff  = "Desactivar automáticamente PCIe (Ahorro de energía)"
AutoLinkDownPhyOff      = "Desactivar PHY automáticamente (Ahorro de energía)"
Battery                 = "Activado, batería"
AcBattery               = "Activado, batería o AC"
GreenEthernet           = "Ethernet ecológico"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Slovak
[Strings.041b]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/p VLAN dodavanje oznaka"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "Kontrolni zbroj na periferiju"
LargesendOffload	= "Slanje velikog na periferiju "
SpeedDuplexMode		= "Brzina i dupleks"
auto_nego		= "Automatsko prilagođivanje"
sd10half		= "10 Mb/s poludupleks"
sd10full		= "10 Mb/s puni dupleks"
sd100half		= "100 Mb/s poludupleks"
sd100full		= "100 Mb/s puni dupleks"
sd1000full		= "1.0 Gb/s puni dupleks"
NetworkAddress		= "Mrežna adresa"
JumboFrame		= "Jumbo okvir"
;TxDescNumber		= "Broj Tx opisnika"
RxDescNumber		= "Broj Rx opisnika"
;TxHPQDescNumber	= "Broj Tx opisnika visokog prioriteta"
FlowControl		= "Kontrola protoka"
;AutoSpeedDown		= "Automatsko smanjivanje brzine"
S5WakeOnLan		= "Isključivanje funkcije Probudi se na mreži nakon isključivanja"
10MbFirst               = "Prvo 10 Mb/s"
100MbFirst              = "Prvo 100 Mb/s"
NotSpeedDown            = "Nema smanjivanja brzine"
WolShutdownLinkSpeed    = "Brzina veze za WOL i isključivanje"
AutoCrossoverDet        = "Automatska detekcija preslušavanja"
Disabled                = "Onemogućeno"
Enabled                 = "Omogućeno"
TxEnabled               = "Tx omogućeno"
RxEnabled               = "Rx omogućeno"
RxTxEnabled             = "Rx & Tx omogućeno"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Mogućnosti Probudi se na mreži"
None                    = "Nema"
PatternMatch            = "Podudarnost obrasca"
MagicPacket             = "Magični paket"
PatternAndMagic         = "Podudarnost obrasca i magični paket"
AutoLinkDownPcieMacOff  = "Automatsko isključivanje PCIe (Štednja energije)"
AutoLinkDownPhyOff      = "Automatsko isključivanje PHY (Štednja energije)"
Battery                 = "Omogućeno, baterija"
AcBattery               = "Omogućeno, baterije ili AC"
GreenEthernet           = "Zeleni Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Swedish
[Strings.041d]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p VLAN-tagging"
;VLanID			= "802.1Q VLAN-identifierare"
ChecksumOffload		= "Avbelasta kontrollsumma"
LargesendOffload	= "Avbelastning för stor överföring"
SpeedDuplexMode		= "Hastighet & duplex"
auto_nego		= "Automatisk förhandling"
sd10half		= "10 Mbps Halv duplex"
sd10full		= "10 Mbps Full duplex"
sd100half		= "100 Mbps Halv duplex"
sd100full		= "100 Mbps Full duplex"
sd1000full		= "1.0 Gbps Full duplex"
NetworkAddress		= "Nätverksadress"
JumboFrame		= "Jumboram"
;TxDescNumber		= "Överföringsbeskrivarens nummer"
RxDescNumber		= "Mottagningsbeskrivarens nummer"
;TxHPQDescNumber	= "Antal beskrivare för högprioritetsöverföring"
FlowControl		= "Flödeskontroll"
;AutoSpeedDown		= "Sänk automatisk hastighet"
S5WakeOnLan		= "Avsluta Wake-on-LAN"
10MbFirst               = "10 Mbps Först"
100MbFirst              = "100 Mbps Först"
NotSpeedDown            = "Not Speed Down"
WolShutdownLinkSpeed    = "Wake-on-LAN och Shutdown Link Speed"
AutoCrossoverDet        = "Automatisk övergångsidentifiering"
Disabled                = "Inaktivera"
Enabled                 = "Aktivera"
TxEnabled               = "Tx aktiverad"
RxEnabled               = "Rx aktiverad"
RxTxEnabled             = "Rx & Tx aktiverad"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Wake-On-Lan Capabilities"
None                    = "None"
PatternMatch            = "Pattern Match"
MagicPacket             = "Magic Packet"
PatternAndMagic         = "Pattern Match & Magic Packet"
AutoLinkDownPcieMacOff  = "Automatisk inaktivering av PCIe (Energisparläge)"
AutoLinkDownPhyOff      = "Automatisk inaktivering av PHY (Energisparläge)"
Battery                 = "Aktiverad, batteri"
AcBattery               = "Aktiverad, batteri eller AC"
GreenEthernet           = "Grönt Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Thai
[Strings.041e]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "การแท็ก VLAN 802.1Q/1p"
;VLanID			= "802.1Q VLAN ID"
ChecksumOffload		= "เช็คซัม ออฟโหลด"
LargesendOffload	= "ส่งออฟโหลดขนาดใหญ่"
SpeedDuplexMode		= "ความเร็ว & ดูเพล็กซ์"
auto_nego		= "การปรับอัตโนมัติ"
sd10half		= "10 Mbps ฮาล์ฟดูเพล็กซ์"
sd10full		= "10 Mbps ฟุลดูเพล็กซ์"
sd100half		= "100 Mbps ฮาล์ฟดูเพล็กซ์"
sd100full		= "100 Mbps ฟุลดูเพล็กซ์"
sd1000full		= "1.0 Gbps ฟุลดูเพล็กซ์"
NetworkAddress		= "เน็ตเวิร์กแอดเดรส"
JumboFrame		= "จัมโบ เฟรม"
;TxDescNumber		= "หมายเลขของตัวอธิบาย Tx"
RxDescNumber		= "หมายเลขของตัวอธิบาย Rx"
;TxHPQDescNumber	= "หมายเลขของตัวอธิบาย Tx ที่มีลำดับความสำคัญสูง"
FlowControl		= "โฟลว์คอนโทรล"
;AutoSpeedDown		= "ลดความเร็วอัตโนมัติ"
S5WakeOnLan		= "การปลุกแลนหลังปิดเครื่อง"
10MbFirst               = "10 Mbps ก่อน"
100MbFirst              = "100 Mbps ก่อน"
NotSpeedDown            = "ไม่ลดความเร็ว"
WolShutdownLinkSpeed    = "ความเร็วลิงค์การปลุกแลน & ปิดเครื่อง"
AutoCrossoverDet        = "การตรวจจับครอสโอเวอร์อัตโนมัติ"
Disabled                = "ปิดทำงาน"
Enabled                 = "เปิดทำงาน"
TxEnabled               = "Tx เช็คซัม"
RxEnabled               = "Rx เช็คซัม"
RxTxEnabled             = "Tx/Rx เช็คซัม"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "คุณสมบัติการปลุกแลน"
None                    = "ไม่มี"
PatternMatch            = "รูปแบบตรง"
MagicPacket             = "เมจิก แพคเก็ต"
PatternAndMagic         = "รูปแบบตรง & เมจิก แพคเก็ต"
AutoLinkDownPcieMacOff  = "ปิดทำงาน PCIe อัตโนมัติ (ประหยัดพลังงาน)"
AutoLinkDownPhyOff      = "ปิดทำงาน PHY อัตโนมัติ (ประหยัดพลังงาน)"
Battery                 = "เปิดทำงาน, แบตเตอรี่"
AcBattery               = "เปิดทำงาน, แบตเตอรี่หรือ AC"
GreenEthernet           = "กรีนอีเธอร์เน็ต"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Turkish
[Strings.041f]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "802.1Q/1p Sanal Yerel Alan Ağı Etiketleme"
;VLanID			= "802.1Q Sanal Yerel Alan Ağ tanımlayıcı"
ChecksumOffload		= "Boşaltmayı Sağla"
LargesendOffload	= "Boşaltmayı Geniş Gönder"
SpeedDuplexMode		= "Hız & İkili"
auto_nego		= "Otomatik Görüşme"
sd10half		= "10 Mbps Yarım İkili"
sd10full		= "10 Mbps Tam İkili"
sd100half		= "100 Mbps Yarım İkili"
sd100full		= "100 Mbps Tam İkili"
sd1000full		= "1.0 Gbps Tam İkili"
NetworkAddress		= "Ağ Adresi"
JumboFrame		= "Jumbo Çerçevesi"
;TxDescNumber		= "İletim Açıklayıcı Sayısı"
RxDescNumber		= "Alım Açıklayıcı Sayısı"
;TxHPQDescNumber	= "Yüksek Öncelikli İletim Açıklayıcı Sayısı"
FlowControl		= "Akış Denetimi"
;AutoSpeedDown		= "Otomatik Yavaşlatma"
S5WakeOnLan		= "Yerel Ağ Üzerinden Kapat"
10MbFirst               = "10 Mbps Önce"
100MbFirst              = "100 Mbps Önce"
NotSpeedDown            = "Yavaşlatma Değil"
WolShutdownLinkSpeed    = "Yerel Ağ Üzerinden Açma & Kapatma Bağlantı Hızı"
AutoCrossoverDet        = "Otomatik Geçiş Algılama"
Disabled                = "Devre dışı bırak"
Enabled                 = "Etkinleştir"
TxEnabled               = "Tx Etkinleştirildi"
RxEnabled               = "Rx Etkinleştirildi"
RxTxEnabled             = "Rx & Tx Etkinleştirildi"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Lan’da Uyan Özellikleri"
None                    = "Yok"
PatternMatch            = "Örnek Eşleşmesi"
MagicPacket             = "Sihirli Paket"
PatternAndMagic         = "Örnek Eşleşmesi & Sihirli Paket"
AutoLinkDownPcieMacOff  = "PCIe’yi (PowerSaving) Otomatik Olarak Devredışı Bırak"
AutoLinkDownPhyOff      = "PHY’yi (PowerSaving) Otomatik Olarak Devredışı Bırak"
Battery                 = "Etkinleştirildi, Pil"
AcBattery               = "Etkinleştirildi, Pil veya AC"
GreenEthernet           = "Yeşil Ethernet"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"

;;Vietnamese
[Strings.042a]
Realtek			= "Realtek Semiconductor Corp."
VLanTagging		= "Gắn nhãn VLAN 802.1Q/1p"
;VLanID			= "ID VLAN 802.1Q"
ChecksumOffload		= "Tải kiểm tra tổng"
LargesendOffload	= "Tải nội dung lớn"
SpeedDuplexMode		= "Tốc độ & Song công"
auto_nego		= "Tự động thỏa thuận"
sd10half		= "10 Mb/giây bán song công"
sd10full		= "10 Mb/giây song công hoàn toàn"
sd100half		= "100 Mb/giây bán song công"
sd100full		= "100 Mb/giây song công hoàn toàn"
sd1000full		= "1 Gb/giây song công hoàn toàn"
NetworkAddress		= "Địa chỉ mạng"
JumboFrame		= "Khung mở rộng"
;TxDescNumber		= "Số nhăn Tx"
RxDescNumber		= "Số nhãn Rx"
;TxHPQDescNumber	= "Số nhăn Tx ưu tiên cao"
FlowControl		= "Kiểm soát lưu lượng"
;AutoSpeedDown		= "Tự động giảm tốc độ"
S5WakeOnLan		= "LAN hiện hành khi tắt máy"
10MbFirst               = "10 Mb/giây trước"
100MbFirst              = "100 Mb/giây trước"
NotSpeedDown            = "Không giảm tốc độ"
WolShutdownLinkSpeed    = "LAN hiện hành & Tắt tốc độ kết nối"
AutoCrossoverDet        = "Tự động bỏ dò tìm"
Disabled                = "Tắt"
Enabled                 = "Bật"
TxEnabled               = "Tx bật"
RxEnabled               = "Rx bật"
RxTxEnabled             = "Rx & Tx bật"
2KBMTU                  = "2KB MTU"
3KBMTU                  = "3KB MTU"
4KBMTU                  = "4KB MTU"
5KBMTU                  = "5KB MTU"
6KBMTU                  = "6KB MTU"
7KBMTU                  = "7KB MTU"
8KBMTU                  = "8KB MTU"
9KBMTU                  = "9KB MTU"
WolCap                  = "Chức năng LAN hiện hành"
None                    = "Không áp dụng"
PatternMatch            = "Khớp kiểu"
MagicPacket             = "Gói ảo"
PatternAndMagic         = "Khớp kiểu & Gói ảo"
AutoLinkDownPcieMacOff  = "Tự động tắt PCIe (Tiết kiệm năng lượng)"
AutoLinkDownPhyOff      = "Tự động tắt PHY (Tiết kiệm năng lượng)"
Battery                 = "Pin bật"
AcBattery               = "Pin hoặc AC bật"
GreenEthernet           = "Ethernet xanh"

;;Source disk name
DISKNAME = "Realtek 10/100/1000 NIC Family all in one NDIS Driver"

RTL8168.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8168C.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168D.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8168DP.DeviceDesc      = "Realtek PCIe GBE Family Controller"
RTL8136.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8102.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8104.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8401.DeviceDesc        = "Realtek PCIe FE Family Controller"
RTL8112.DeviceDesc        = "Realtek PCIe GBE Family Controller"
RTL8112L.DeviceDesc       = "Realtek PCIe GBE Family Controller"
RTL8131.DeviceDesc        = "Realtek PCIe FE Family Controller"

;;NT service name
Rtlnic.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NT Driver"
Rtlnicxp.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP Driver"
Rtlnicx64.Service.DispName    = "Realtek 10/100/1000 PCI-E NIC Family NDIS XP(x64) Driver"