1. Put all files under EXE folder into Demo\HYKBStatsDemo\HYKBStatsDemo folder
2. The firmware files, keymap files are hardcoded in the demo program.
3. To test the firmware update, 2 firmware files (same features, but with different versions), 
   L2326V151.bin and L2326V152.bin are provided in the demo project folder.
4. The keymap file must be created by selecting KB66-Dual in Matrix Maker.